From 22774ebfc4073fd3c0fc729e2ae1e0e762ec127e Mon Sep 17 00:00:00 2001
From: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Date: Sun, 16 Oct 2022 09:15:04 +0300
Subject: [PATCH] media: dt-bindings: Convert imx290.txt to YAML

Upstream commit a96dfea1df25

Convert the Sony IMX290 DT binding from text to YAML. Add Manivannan as
a maintainer given that he is listed in MAINTAINERS for the file, as
volunteering myself.

The name of the input clock, "xclk", is wrong as the hardware manual
names it INCK. As the device has a single clock, the name could be
omitted, but that would require a corresponding change to the driver and
is thus a candidate for further patches.

Signed-off-by: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Signed-off-by: Sakari Ailus <sakari.ailus@linux.intel.com>
---
 .../devicetree/bindings/media/i2c/imx290.txt  |  57 --------
 .../bindings/media/i2c/sony,imx290.yaml       | 129 ++++++++++++++++++
 MAINTAINERS                                   |   2 +-
 3 files changed, 130 insertions(+), 58 deletions(-)
 delete mode 100644 Documentation/devicetree/bindings/media/i2c/imx290.txt
 create mode 100644 Documentation/devicetree/bindings/media/i2c/sony,imx290.yaml

--- a/Documentation/devicetree/bindings/media/i2c/imx290.txt
+++ /dev/null
@@ -1,57 +0,0 @@
-* Sony IMX290 1/2.8-Inch CMOS Image Sensor
-
-The Sony IMX290 is a 1/2.8-Inch CMOS Solid-state image sensor with
-Square Pixel for Color Cameras. It is programmable through I2C and 4-wire
-interfaces. The sensor output is available via CMOS logic parallel SDR output,
-Low voltage LVDS DDR output and CSI-2 serial data output. The CSI-2 bus is the
-default. No bindings have been defined for the other busses.
-
-Required Properties:
-- compatible: Should be "sony,imx290"
-- reg: I2C bus address of the device
-- clocks: Reference to the xclk clock.
-- clock-names: Should be "xclk".
-- clock-frequency: Frequency of the xclk clock in Hz.
-- vdddo-supply: Sensor digital IO regulator.
-- vdda-supply: Sensor analog regulator.
-- vddd-supply: Sensor digital core regulator.
-
-Optional Properties:
-- reset-gpios: Sensor reset GPIO
-
-The imx290 device node should contain one 'port' child node with
-an 'endpoint' subnode. For further reading on port node refer to
-Documentation/devicetree/bindings/media/video-interfaces.txt.
-
-Required Properties on endpoint:
-- data-lanes: check ../video-interfaces.txt
-- link-frequencies: check ../video-interfaces.txt
-- remote-endpoint: check ../video-interfaces.txt
-
-Example:
-	&i2c1 {
-		...
-		imx290: camera-sensor@1a {
-			compatible = "sony,imx290";
-			reg = <0x1a>;
-
-			reset-gpios = <&msmgpio 35 GPIO_ACTIVE_LOW>;
-			pinctrl-names = "default";
-			pinctrl-0 = <&camera_rear_default>;
-
-			clocks = <&gcc GCC_CAMSS_MCLK0_CLK>;
-			clock-names = "xclk";
-			clock-frequency = <37125000>;
-
-			vdddo-supply = <&camera_vdddo_1v8>;
-			vdda-supply = <&camera_vdda_2v8>;
-			vddd-supply = <&camera_vddd_1v5>;
-
-			port {
-				imx290_ep: endpoint {
-					data-lanes = <1 2 3 4>;
-					link-frequencies = /bits/ 64 <445500000>;
-					remote-endpoint = <&csiphy0_ep>;
-				};
-			};
-		};
--- /dev/null
+++ b/Documentation/devicetree/bindings/media/i2c/sony,imx290.yaml
@@ -0,0 +1,129 @@
+# SPDX-License-Identifier: (GPL-2.0 OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/media/i2c/sony,imx290.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Sony IMX290 1/2.8-Inch CMOS Image Sensor
+
+maintainers:
+  - Manivannan Sadhasivam <manivannan.sadhasivam@linaro.org>
+  - Laurent Pinchart <laurent.pinchart@ideasonboard.com>
+
+description: |-
+  The Sony IMX290 is a 1/2.8-Inch CMOS Solid-state image sensor with Square
+  Pixel for Color Cameras. It is programmable through I2C and 4-wire
+  interfaces. The sensor output is available via CMOS logic parallel SDR
+  output, Low voltage LVDS DDR output and CSI-2 serial data output. The CSI-2
+  bus is the default. No bindings have been defined for the other busses.
+
+properties:
+  compatible:
+    enum:
+      - sony,imx290
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    maxItems: 1
+
+  clock-names:
+    description: Input clock (37.125 MHz or 74.25 MHz)
+    items:
+      - const: xclk
+
+  clock-frequency:
+    description: Frequency of the xclk clock in Hz
+
+  vdda-supply:
+    description: Analog power supply (2.9V)
+
+  vddd-supply:
+    description: Digital core power supply (1.2V)
+
+  vdddo-supply:
+    description: Digital I/O power supply (1.8V)
+
+  reset-gpios:
+    description: Sensor reset (XCLR) GPIO
+    maxItems: 1
+
+  port:
+    $ref: /schemas/graph.yaml#/$defs/port-base
+    description: |
+      Video output port
+
+    properties:
+      endpoint:
+        $ref: /schemas/media/video-interfaces.yaml#
+        unevaluatedProperties: false
+
+        properties:
+          data-lanes:
+            anyOf:
+              - items:
+                  - const: 1
+                  - const: 2
+              - items:
+                  - const: 1
+                  - const: 2
+                  - const: 3
+                  - const: 4
+
+          link-frequencies: true
+
+        required:
+          - data-lanes
+          - link-frequencies
+
+    additionalProperties: false
+
+required:
+  - compatible
+  - reg
+  - clocks
+  - clock-names
+  - clock-frequency
+  - vdda-supply
+  - vddd-supply
+  - vdddo-supply
+  - port
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/gpio/gpio.h>
+
+    i2c {
+        #address-cells = <1>;
+        #size-cells = <0>;
+
+        imx290: camera-sensor@1a {
+            compatible = "sony,imx290";
+            reg = <0x1a>;
+
+            pinctrl-names = "default";
+            pinctrl-0 = <&camera_rear_default>;
+
+            clocks = <&gcc 90>;
+            clock-names = "xclk";
+            clock-frequency = <37125000>;
+
+            vdddo-supply = <&camera_vdddo_1v8>;
+            vdda-supply = <&camera_vdda_2v8>;
+            vddd-supply = <&camera_vddd_1v5>;
+
+            reset-gpios = <&msmgpio 35 GPIO_ACTIVE_LOW>;
+
+            port {
+                imx290_ep: endpoint {
+                    data-lanes = <1 2 3 4>;
+                    link-frequencies = /bits/ 64 <445500000>;
+                    remote-endpoint = <&csiphy0_ep>;
+                };
+            };
+        };
+    };
+...
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -19278,7 +19278,7 @@ M:	Manivannan Sadhasivam <manivannan.sad
 L:	linux-media@vger.kernel.org
 S:	Maintained
 T:	git git://linuxtv.org/media_tree.git
-F:	Documentation/devicetree/bindings/media/i2c/imx290.txt
+F:	Documentation/devicetree/bindings/media/i2c/sony,imx290.yaml
 F:	drivers/media/i2c/imx290.c
 
 SONY IMX296 SENSOR DRIVER
