From 27b389d9f62c2174f95fe4002b11e77d4cb3ce80 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?N=C3=ADcolas=20F=2E=20R=2E=20A=2E=20Prado?=
 <nfraprado@collabora.com>
Date: Thu, 6 Jul 2023 11:37:32 -0400
Subject: [PATCH 25/42] thermal/drivers/mediatek/lvts_thermal: Handle IRQ on
 all controllers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

There is a single IRQ handler for each LVTS thermal domain, and it is
supposed to check each of its underlying controllers for the origin of
the interrupt and clear its status. However due to a typo, only the
first controller was ever being handled, which resulted in the interrupt
never being cleared when it happened on the other controllers. Add the
missing index so interrupts are handled for all controllers.

Fixes: f5f633b18234 ("thermal/drivers/mediatek: Add the Low Voltage Thermal Sensor driver")
Reviewed-by: Matthias Brugger <matthias.bgg@gmail.com>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>
Tested-by: Chen-Yu Tsai <wenst@chromium.org>
Signed-off-by: Nícolas F. R. A. Prado <nfraprado@collabora.com>
Reviewed-by: Alexandre Mergnat <amergnat@baylibre.com>
Signed-off-by: Daniel Lezcano <daniel.lezcano@linaro.org>
Link: https://lore.kernel.org/r/20230706153823.201943-2-nfraprado@collabora.com
---
 drivers/thermal/mediatek/lvts_thermal.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/thermal/mediatek/lvts_thermal.c
+++ b/drivers/thermal/mediatek/lvts_thermal.c
@@ -451,7 +451,7 @@ static irqreturn_t lvts_irq_handler(int
 
 	for (i = 0; i < lvts_td->num_lvts_ctrl; i++) {
 
-		aux = lvts_ctrl_irq_handler(lvts_td->lvts_ctrl);
+		aux = lvts_ctrl_irq_handler(&lvts_td->lvts_ctrl[i]);
 		if (aux != IRQ_HANDLED)
 			continue;
 
