From 02767440e1dda9861a11ca1dbe0f19a760b1d5c2 Mon Sep 17 00:00:00 2001
From: Hayes Wang <hayeswang@realtek.com>
Date: Thu, 19 Jan 2023 15:40:43 +0800
Subject: [PATCH] r8152: reduce the control transfer of rtl8152_get_version()

Reduce the control transfer by moving calling rtl8152_get_version() in
rtl8152_probe(). This could prevent from calling rtl8152_get_version()
for unnecessary situations. For example, after setting config #2 for the
device, there are two interfaces and rtl8152_probe() may be called
twice. However, we don't need to call rtl8152_get_version() for this
situation.

Signed-off-by: Hayes Wang <hayeswang@realtek.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/usb/r8152.c | 9 +++++----
 1 file changed, 5 insertions(+), 4 deletions(-)

--- a/drivers/net/usb/r8152.c
+++ b/drivers/net/usb/r8152.c
@@ -9638,20 +9638,21 @@ static int rtl8152_probe(struct usb_inte
 			 const struct usb_device_id *id)
 {
 	struct usb_device *udev = interface_to_usbdev(intf);
-	u8 version = rtl8152_get_version(intf);
 	struct r8152 *tp;
 	struct net_device *netdev;
+	u8 version;
 	int ret;
 
-	if (version == RTL_VER_UNKNOWN)
-		return -ENODEV;
-
 	if (intf->cur_altsetting->desc.bInterfaceClass != USB_CLASS_VENDOR_SPEC)
 		return -ENODEV;
 
 	if (!rtl_check_vendor_ok(intf))
 		return -ENODEV;
 
+	version = rtl8152_get_version(intf);
+	if (version == RTL_VER_UNKNOWN)
+		return -ENODEV;
+
 	usb_reset_device(udev);
 	netdev = alloc_etherdev(sizeof(struct r8152));
 	if (!netdev) {
