From a04a6eb3b4d112f3600bbd783249f24a43797e7a Mon Sep 17 00:00:00 2001
From: Xingyu Wu <xingyu.wu@starfivetech.com>
Date: Thu, 18 May 2023 18:12:31 +0800
Subject: [PATCH 057/122] reset: starfive: jh7110: Add StarFive STG/ISP/VOUT
 resets support

Add new struct members and auxiliary_device_id of resets to support
System-Top-Group, Image-Signal-Process and Video-Output on the StarFive
JH7110 SoC.

Signed-off-by: Xingyu Wu <xingyu.wu@starfivetech.com>
---
 .../reset/starfive/reset-starfive-jh7110.c    | 30 +++++++++++++++++++
 1 file changed, 30 insertions(+)

--- a/drivers/reset/starfive/reset-starfive-jh7110.c
+++ b/drivers/reset/starfive/reset-starfive-jh7110.c
@@ -31,6 +31,24 @@ static const struct jh7110_reset_info jh
 	.status_offset = 0x3C,
 };
 
+static const struct jh7110_reset_info jh7110_stg_info = {
+	.nr_resets = JH7110_STGRST_END,
+	.assert_offset = 0x74,
+	.status_offset = 0x78,
+};
+
+static const struct jh7110_reset_info jh7110_isp_info = {
+	.nr_resets = JH7110_ISPRST_END,
+	.assert_offset = 0x38,
+	.status_offset = 0x3C,
+};
+
+static const struct jh7110_reset_info jh7110_vout_info = {
+	.nr_resets = JH7110_VOUTRST_END,
+	.assert_offset = 0x48,
+	.status_offset = 0x4C,
+};
+
 static int jh7110_reset_probe(struct auxiliary_device *adev,
 			      const struct auxiliary_device_id *id)
 {
@@ -58,6 +76,18 @@ static const struct auxiliary_device_id
 		.name = "clk_starfive_jh7110_sys.rst-aon",
 		.driver_data = (kernel_ulong_t)&jh7110_aon_info,
 	},
+	{
+		.name = "clk_starfive_jh7110_sys.rst-stg",
+		.driver_data = (kernel_ulong_t)&jh7110_stg_info,
+	},
+	{
+		.name = "clk_starfive_jh7110_sys.rst-isp",
+		.driver_data = (kernel_ulong_t)&jh7110_isp_info,
+	},
+	{
+		.name = "clk_starfive_jh7110_sys.rst-vo",
+		.driver_data = (kernel_ulong_t)&jh7110_vout_info,
+	},
 	{ /* sentinel */ }
 };
 MODULE_DEVICE_TABLE(auxiliary, jh7110_reset_ids);
