From e718fc8f42a900b7b07b806ddfdb8c2b7a1aa3b1 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Fri, 10 Mar 2023 16:57:29 +0000
Subject: [PATCH] vc04_services: bcm2835_codec: Set MPEG2_LEVEL control
 to READ_ONLY

V4L2_CID_MPEG_VIDEO_MPEG2_LEVEL  was missed from
"vc04_services: bcm2835_codec: Ignore READ_ONLY ctrls in s_ctrl"

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/staging/vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/staging/vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c
+++ b/drivers/staging/vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c
@@ -3246,6 +3246,7 @@ static void dec_add_profile_ctrls(struct
 							BIT(V4L2_MPEG_VIDEO_MPEG2_LEVEL_HIGH_1440) |
 							BIT(V4L2_MPEG_VIDEO_MPEG2_LEVEL_HIGH)),
 						      V4L2_MPEG_VIDEO_MPEG2_LEVEL_MAIN);
+			ctrl->flags |= V4L2_CTRL_FLAG_READ_ONLY;
 			ctrl = v4l2_ctrl_new_std_menu(hdl, &bcm2835_codec_ctrl_ops,
 						      V4L2_CID_MPEG_VIDEO_MPEG2_PROFILE,
 						      V4L2_MPEG_VIDEO_MPEG2_PROFILE_MAIN,
