From 9da6b4ad7ee76da4d274f305412fc6f2bc95c91c Mon Sep 17 00:00:00 2001
From: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Date: Sun, 16 Oct 2022 09:15:05 +0300
Subject: [PATCH] media: i2c: imx290: Use device lock for the control
 handler

Upstream commit 08878cbc0cbf.

The link frequency and pixel rate controls are set without holding the
control handler lock, resulting in kernel warnings. As the value of
those controls depend on the format, the simplest fix is to use the
device lock for the control handler.

Signed-off-by: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Reviewed-by: Alexander Stein <alexander.stein@ew.tq-group.com>
Signed-off-by: Sakari Ailus <sakari.ailus@linux.intel.com>
---
 drivers/media/i2c/imx290.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/media/i2c/imx290.c
+++ b/drivers/media/i2c/imx290.c
@@ -1043,6 +1043,7 @@ static int imx290_probe(struct i2c_clien
 	imx290_entity_init_cfg(&imx290->sd, NULL);
 
 	v4l2_ctrl_handler_init(&imx290->ctrls, 4);
+	imx290->ctrls.lock = &imx290->lock;
 
 	v4l2_ctrl_new_std(&imx290->ctrls, &imx290_ctrl_ops,
 			  V4L2_CID_GAIN, 0, 72, 1, 0);
