#include "bcm3368.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Netgear CVG834G";
	compatible = "netgear,cvg834g", "brcm,bcm3368";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 5 0>;
			default-state = "on";
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x010000>;
			read-only;
		};

		linux@10000 {
			label = "linux";
			reg = <0x010000 0x3e0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@3f0000 {
			label = "nvram";
			reg = <0x3f0000 0x010000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&uart1 {
	status = "okay";
};
