From 24a303eec794e5a1e8479430191237c2ebdd23d9 Mon Sep 17 00:00:00 2001
From: Lee Jackson <lee.jackson@arducam.com>
Date: Wed, 22 Mar 2023 16:24:19 +0800
Subject: [PATCH] dtoverlays: Reduce the link-frequencies of IMX519

Modify the link-frequencies of IMX519 to 408000000.

Signed-off-by: Lee Jackson <lee.jackson@arducam.com>
---
 arch/arm/boot/dts/overlays/imx519.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/imx519.dtsi
+++ b/arch/arm/boot/dts/overlays/imx519.dtsi
@@ -21,7 +21,7 @@ cam_node: imx519@1a {
 			data-lanes = <1 2>;
 			clock-noncontinuous;
 			link-frequencies =
-				/bits/ 64 <493500000>;
+				/bits/ 64 <408000000>;
 		};
 	};
 };
