From 73cbfad9296eed004992806e056db5b48583ca41 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Alexis=20Lothor=C3=A9?= <alexis.lothore@bootlin.com>
Date: Mon, 29 May 2023 10:02:42 +0200
Subject: [PATCH 2/6] net: dsa: mv88e6xxx: use mv88e6xxx_phy_is_internal in
 mv88e6xxx_port_ppu_updates
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Make sure to use existing helper to get internal PHYs count instead of
redoing it manually

Signed-off-by: Alexis Lothoré <alexis.lothore@bootlin.com>
Reviewed-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/mv88e6xxx/chip.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -484,7 +484,7 @@ static int mv88e6xxx_port_ppu_updates(st
 	 * report whether the port is internal.
 	 */
 	if (chip->info->family == MV88E6XXX_FAMILY_6250)
-		return port < chip->info->num_internal_phys;
+		return mv88e6xxx_phy_is_internal(chip, port);
 
 	err = mv88e6xxx_port_read(chip, port, MV88E6XXX_PORT_STS, &reg);
 	if (err) {
