// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "rakwireless,rak633", "mediatek,mt7628an-soc";
	model = "Rakwireless RAK633";

	leds {
		compatible = "gpio-leds";

		wifi {
			label = "blue:wifi";
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};
	};
};

&state_default {
	wled_an {
		groups = "wled_an";
		function = "gpio";
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x400>;
					};

					macaddr_factory_28: macaddr@28 {
						reg = <0x28 0x6>;
					};
				};
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&i2c {
	status = "okay";
};

&i2s {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&uart2 {
	status = "okay";
};

&gdma {
	status = "okay";
};

&ethernet {
	nvmem-cells = <&macaddr_factory_28>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	nvmem-cells = <&eeprom_factory_0>;
	nvmem-cell-names = "eeprom";
};
