From d68a283bfc39aeed2a51c67804e014bf4b35c7e1 Mon Sep 17 00:00:00 2001
From: Jeff Johnson <quic_jjohnson@quicinc.com>
Date: Tue, 22 Aug 2023 07:50:49 -0700
Subject: [PATCH] wifi: ath11k: Fix a few spelling errors

Fix a few issues flagged by 'codespell'.

Signed-off-by: Jeff Johnson <quic_jjohnson@quicinc.com>
Acked-by: Randy Dunlap <rdunlap@infradead.org>
Signed-off-by: Kalle Valo <quic_kvalo@quicinc.com>
Link: https://lore.kernel.org/r/20230822-ath_spelling-v1-2-8e2698759564@quicinc.com
---
 drivers/net/wireless/ath/ath11k/dp.h    | 2 +-
 drivers/net/wireless/ath/ath11k/dp_rx.c | 2 +-
 drivers/net/wireless/ath/ath11k/dp_tx.c | 2 +-
 3 files changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/net/wireless/ath/ath11k/dp.h
+++ b/drivers/net/wireless/ath/ath11k/dp.h
@@ -635,7 +635,7 @@ enum htt_ppdu_stats_tag_type {
  *          b'24    - status_swap: 1 is to swap status TLV
  *          b'25    - pkt_swap:  1 is to swap packet TLV
  *          b'26:31 - rsvd1:  reserved for future use
- * dword1 - b'0:16  - ring_buffer_size: size of bufferes referenced by rx ring,
+ * dword1 - b'0:16  - ring_buffer_size: size of buffers referenced by rx ring,
  *                    in byte units.
  *                    Valid only for HW_TO_SW_RING and SW_TO_HW_RING
  *        - b'16:31 - rsvd2: Reserved for future use
--- a/drivers/net/wireless/ath/ath11k/dp_rx.c
+++ b/drivers/net/wireless/ath/ath11k/dp_rx.c
@@ -3423,7 +3423,7 @@ static int ath11k_dp_rx_h_defrag_reo_rei
 	ath11k_hal_rx_buf_addr_info_set(msdu0, paddr, cookie,
 					ab->hw_params.hal_params->rx_buf_rbm);
 
-	/* Fill mpdu details into reo entrace ring */
+	/* Fill mpdu details into reo entrance ring */
 	srng = &ab->hal.srng_list[ab->dp.reo_reinject_ring.ring_id];
 
 	spin_lock_bh(&srng->lock);
--- a/drivers/net/wireless/ath/ath11k/dp_tx.c
+++ b/drivers/net/wireless/ath/ath11k/dp_tx.c
@@ -238,7 +238,7 @@ tcl_ring_sel:
 		spin_unlock_bh(&tcl_ring->lock);
 		ret = -ENOMEM;
 
-		/* Checking for available tcl descritors in another ring in
+		/* Checking for available tcl descriptors in another ring in
 		 * case of failure due to full tcl ring now, is better than
 		 * checking this ring earlier for each pkt tx.
 		 * Restart ring selection if some rings are not checked yet.
