From f8ed4088ed9c61ae92193da6130d04c37e7b19f2 Mon Sep 17 00:00:00 2001
From: Frank Wunderlich <frank-w@public-files.de>
Date: Sun, 20 Aug 2023 17:31:33 +0200
Subject: [PATCH 20/22] arm64: dts: mt7986: define 3W max power to both SFP on
 BPI-R3

All SFP power supplies are connected to the system VDD33 which is 3v3/8A.
Set 3A per SFP slot to allow SFPs work which need more power than the
default 1W.

Fixes: 8e01fb15b815 ("arm64: dts: mt7986: add Bananapi R3")
Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
---
 arch/arm64/boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/arm64/boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts
@@ -126,6 +126,7 @@
 		compatible = "sff,sfp";
 		i2c-bus = <&i2c_sfp1>;
 		los-gpios = <&pio 46 GPIO_ACTIVE_HIGH>;
+		maximum-power-milliwatt = <3000>;
 		mod-def0-gpios = <&pio 49 GPIO_ACTIVE_LOW>;
 		tx-disable-gpios = <&pio 20 GPIO_ACTIVE_HIGH>;
 		tx-fault-gpios = <&pio 7 GPIO_ACTIVE_HIGH>;
@@ -137,6 +138,7 @@
 		i2c-bus = <&i2c_sfp2>;
 		los-gpios = <&pio 31 GPIO_ACTIVE_HIGH>;
 		mod-def0-gpios = <&pio 47 GPIO_ACTIVE_LOW>;
+		maximum-power-milliwatt = <3000>;
 		tx-disable-gpios = <&pio 15 GPIO_ACTIVE_HIGH>;
 		tx-fault-gpios = <&pio 48 GPIO_ACTIVE_HIGH>;
 	};
