From 5d0fad48d2dec175ecb999974b94203c577973ef Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Wed, 8 May 2024 11:43:34 +0100
Subject: [PATCH] net: ethernet: mediatek: split tx and rx fields in
 mtk_soc_data struct

Split tx and rx fields in mtk_soc_data struct. This is a preliminary
patch to roll back to ADMAv1 for MT7986 and MT7981 SoC in order to fix a
hw hang if the device receives a corrupted packet when using ADMAv2.0.

Fixes: 197c9e9b17b1 ("net: ethernet: mtk_eth_soc: introduce support for mt7986 chipset")
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Przemek Kitszel <przemyslaw.kitszel@intel.com>
Link: https://lore.kernel.org/r/70a799b1f060ec2f57883e88ccb420ac0fb0abb5.1715164770.git.daniel@makrotopia.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 210 ++++++++++++--------
 drivers/net/ethernet/mediatek/mtk_eth_soc.h |  29 +--
 2 files changed, 139 insertions(+), 100 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1138,7 +1138,7 @@ static int mtk_init_fq_dma(struct mtk_et
 		eth->scratch_ring = eth->sram_base;
 	else
 		eth->scratch_ring = dma_alloc_coherent(eth->dma_dev,
-						       cnt * soc->txrx.txd_size,
+						       cnt * soc->tx.desc_size,
 						       &eth->phy_scratch_ring,
 						       GFP_KERNEL);
 	if (unlikely(!eth->scratch_ring))
@@ -1154,16 +1154,16 @@ static int mtk_init_fq_dma(struct mtk_et
 	if (unlikely(dma_mapping_error(eth->dma_dev, dma_addr)))
 		return -ENOMEM;
 
-	phy_ring_tail = eth->phy_scratch_ring + soc->txrx.txd_size * (cnt - 1);
+	phy_ring_tail = eth->phy_scratch_ring + soc->tx.desc_size * (cnt - 1);
 
 	for (i = 0; i < cnt; i++) {
 		struct mtk_tx_dma_v2 *txd;
 
-		txd = eth->scratch_ring + i * soc->txrx.txd_size;
+		txd = eth->scratch_ring + i * soc->tx.desc_size;
 		txd->txd1 = dma_addr + i * MTK_QDMA_PAGE_SIZE;
 		if (i < cnt - 1)
 			txd->txd2 = eth->phy_scratch_ring +
-				    (i + 1) * soc->txrx.txd_size;
+				    (i + 1) * soc->tx.desc_size;
 
 		txd->txd3 = TX_DMA_PLEN0(MTK_QDMA_PAGE_SIZE);
 		txd->txd4 = 0;
@@ -1412,7 +1412,7 @@ static int mtk_tx_map(struct sk_buff *sk
 	if (itxd == ring->last_free)
 		return -ENOMEM;
 
-	itx_buf = mtk_desc_to_tx_buf(ring, itxd, soc->txrx.txd_size);
+	itx_buf = mtk_desc_to_tx_buf(ring, itxd, soc->tx.desc_size);
 	memset(itx_buf, 0, sizeof(*itx_buf));
 
 	txd_info.addr = dma_map_single(eth->dma_dev, skb->data, txd_info.size,
@@ -1453,7 +1453,7 @@ static int mtk_tx_map(struct sk_buff *sk
 
 			memset(&txd_info, 0, sizeof(struct mtk_tx_dma_desc_info));
 			txd_info.size = min_t(unsigned int, frag_size,
-					      soc->txrx.dma_max_len);
+					      soc->tx.dma_max_len);
 			txd_info.qid = queue;
 			txd_info.last = i == skb_shinfo(skb)->nr_frags - 1 &&
 					!(frag_size - txd_info.size);
@@ -1466,7 +1466,7 @@ static int mtk_tx_map(struct sk_buff *sk
 			mtk_tx_set_dma_desc(dev, txd, &txd_info);
 
 			tx_buf = mtk_desc_to_tx_buf(ring, txd,
-						    soc->txrx.txd_size);
+						    soc->tx.desc_size);
 			if (new_desc)
 				memset(tx_buf, 0, sizeof(*tx_buf));
 			tx_buf->data = (void *)MTK_DMA_DUMMY_DESC;
@@ -1509,7 +1509,7 @@ static int mtk_tx_map(struct sk_buff *sk
 	} else {
 		int next_idx;
 
-		next_idx = NEXT_DESP_IDX(txd_to_idx(ring, txd, soc->txrx.txd_size),
+		next_idx = NEXT_DESP_IDX(txd_to_idx(ring, txd, soc->tx.desc_size),
 					 ring->dma_size);
 		mtk_w32(eth, next_idx, MT7628_TX_CTX_IDX0);
 	}
@@ -1518,7 +1518,7 @@ static int mtk_tx_map(struct sk_buff *sk
 
 err_dma:
 	do {
-		tx_buf = mtk_desc_to_tx_buf(ring, itxd, soc->txrx.txd_size);
+		tx_buf = mtk_desc_to_tx_buf(ring, itxd, soc->tx.desc_size);
 
 		/* unmap dma */
 		mtk_tx_unmap(eth, tx_buf, NULL, false);
@@ -1543,7 +1543,7 @@ static int mtk_cal_txd_req(struct mtk_et
 		for (i = 0; i < skb_shinfo(skb)->nr_frags; i++) {
 			frag = &skb_shinfo(skb)->frags[i];
 			nfrags += DIV_ROUND_UP(skb_frag_size(frag),
-					       eth->soc->txrx.dma_max_len);
+					       eth->soc->tx.dma_max_len);
 		}
 	} else {
 		nfrags += skb_shinfo(skb)->nr_frags;
@@ -1650,7 +1650,7 @@ static struct mtk_rx_ring *mtk_get_rx_ri
 
 		ring = &eth->rx_ring[i];
 		idx = NEXT_DESP_IDX(ring->calc_idx, ring->dma_size);
-		rxd = ring->dma + idx * eth->soc->txrx.rxd_size;
+		rxd = ring->dma + idx * eth->soc->rx.desc_size;
 		if (rxd->rxd2 & RX_DMA_DONE) {
 			ring->calc_idx_update = true;
 			return ring;
@@ -1818,7 +1818,7 @@ static int mtk_xdp_submit_frame(struct m
 	}
 	htxd = txd;
 
-	tx_buf = mtk_desc_to_tx_buf(ring, txd, soc->txrx.txd_size);
+	tx_buf = mtk_desc_to_tx_buf(ring, txd, soc->tx.desc_size);
 	memset(tx_buf, 0, sizeof(*tx_buf));
 	htx_buf = tx_buf;
 
@@ -1837,7 +1837,7 @@ static int mtk_xdp_submit_frame(struct m
 				goto unmap;
 
 			tx_buf = mtk_desc_to_tx_buf(ring, txd,
-						    soc->txrx.txd_size);
+						    soc->tx.desc_size);
 			memset(tx_buf, 0, sizeof(*tx_buf));
 			n_desc++;
 		}
@@ -1875,7 +1875,7 @@ static int mtk_xdp_submit_frame(struct m
 	} else {
 		int idx;
 
-		idx = txd_to_idx(ring, txd, soc->txrx.txd_size);
+		idx = txd_to_idx(ring, txd, soc->tx.desc_size);
 		mtk_w32(eth, NEXT_DESP_IDX(idx, ring->dma_size),
 			MT7628_TX_CTX_IDX0);
 	}
@@ -1886,7 +1886,7 @@ static int mtk_xdp_submit_frame(struct m
 
 unmap:
 	while (htxd != txd) {
-		tx_buf = mtk_desc_to_tx_buf(ring, htxd, soc->txrx.txd_size);
+		tx_buf = mtk_desc_to_tx_buf(ring, htxd, soc->tx.desc_size);
 		mtk_tx_unmap(eth, tx_buf, NULL, false);
 
 		htxd->txd3 = TX_DMA_LS0 | TX_DMA_OWNER_CPU;
@@ -2017,7 +2017,7 @@ static int mtk_poll_rx(struct napi_struc
 			goto rx_done;
 
 		idx = NEXT_DESP_IDX(ring->calc_idx, ring->dma_size);
-		rxd = ring->dma + idx * eth->soc->txrx.rxd_size;
+		rxd = ring->dma + idx * eth->soc->rx.desc_size;
 		data = ring->data[idx];
 
 		if (!mtk_rx_get_desc(eth, &trxd, rxd))
@@ -2152,7 +2152,7 @@ static int mtk_poll_rx(struct napi_struc
 			rxdcsum = &trxd.rxd4;
 		}
 
-		if (*rxdcsum & eth->soc->txrx.rx_dma_l4_valid)
+		if (*rxdcsum & eth->soc->rx.dma_l4_valid)
 			skb->ip_summed = CHECKSUM_UNNECESSARY;
 		else
 			skb_checksum_none_assert(skb);
@@ -2276,7 +2276,7 @@ static int mtk_poll_tx_qdma(struct mtk_e
 			break;
 
 		tx_buf = mtk_desc_to_tx_buf(ring, desc,
-					    eth->soc->txrx.txd_size);
+					    eth->soc->tx.desc_size);
 		if (!tx_buf->data)
 			break;
 
@@ -2327,7 +2327,7 @@ static int mtk_poll_tx_pdma(struct mtk_e
 		}
 		mtk_tx_unmap(eth, tx_buf, &bq, true);
 
-		desc = ring->dma + cpu * eth->soc->txrx.txd_size;
+		desc = ring->dma + cpu * eth->soc->tx.desc_size;
 		ring->last_free = desc;
 		atomic_inc(&ring->free_count);
 
@@ -2417,7 +2417,7 @@ static int mtk_napi_rx(struct napi_struc
 	do {
 		int rx_done;
 
-		mtk_w32(eth, eth->soc->txrx.rx_irq_done_mask,
+		mtk_w32(eth, eth->soc->rx.irq_done_mask,
 			reg_map->pdma.irq_status);
 		rx_done = mtk_poll_rx(napi, budget - rx_done_total, eth);
 		rx_done_total += rx_done;
@@ -2433,10 +2433,10 @@ static int mtk_napi_rx(struct napi_struc
 			return budget;
 
 	} while (mtk_r32(eth, reg_map->pdma.irq_status) &
-		 eth->soc->txrx.rx_irq_done_mask);
+		 eth->soc->rx.irq_done_mask);
 
 	if (napi_complete_done(napi, rx_done_total))
-		mtk_rx_irq_enable(eth, eth->soc->txrx.rx_irq_done_mask);
+		mtk_rx_irq_enable(eth, eth->soc->rx.irq_done_mask);
 
 	return rx_done_total;
 }
@@ -2445,7 +2445,7 @@ static int mtk_tx_alloc(struct mtk_eth *
 {
 	const struct mtk_soc_data *soc = eth->soc;
 	struct mtk_tx_ring *ring = &eth->tx_ring;
-	int i, sz = soc->txrx.txd_size;
+	int i, sz = soc->tx.desc_size;
 	struct mtk_tx_dma_v2 *txd;
 	int ring_size;
 	u32 ofs, val;
@@ -2568,14 +2568,14 @@ static void mtk_tx_clean(struct mtk_eth
 	}
 	if (!MTK_HAS_CAPS(soc->caps, MTK_SRAM) && ring->dma) {
 		dma_free_coherent(eth->dma_dev,
-				  ring->dma_size * soc->txrx.txd_size,
+				  ring->dma_size * soc->tx.desc_size,
 				  ring->dma, ring->phys);
 		ring->dma = NULL;
 	}
 
 	if (ring->dma_pdma) {
 		dma_free_coherent(eth->dma_dev,
-				  ring->dma_size * soc->txrx.txd_size,
+				  ring->dma_size * soc->tx.desc_size,
 				  ring->dma_pdma, ring->phys_pdma);
 		ring->dma_pdma = NULL;
 	}
@@ -2630,15 +2630,15 @@ static int mtk_rx_alloc(struct mtk_eth *
 	if (!MTK_HAS_CAPS(eth->soc->caps, MTK_SRAM) ||
 	    rx_flag != MTK_RX_FLAGS_NORMAL) {
 		ring->dma = dma_alloc_coherent(eth->dma_dev,
-					       rx_dma_size * eth->soc->txrx.rxd_size,
-					       &ring->phys, GFP_KERNEL);
+				rx_dma_size * eth->soc->rx.desc_size,
+				&ring->phys, GFP_KERNEL);
 	} else {
 		struct mtk_tx_ring *tx_ring = &eth->tx_ring;
 
 		ring->dma = tx_ring->dma + tx_ring_size *
-			    eth->soc->txrx.txd_size * (ring_no + 1);
+			    eth->soc->tx.desc_size * (ring_no + 1);
 		ring->phys = tx_ring->phys + tx_ring_size *
-			     eth->soc->txrx.txd_size * (ring_no + 1);
+			     eth->soc->tx.desc_size * (ring_no + 1);
 	}
 
 	if (!ring->dma)
@@ -2649,7 +2649,7 @@ static int mtk_rx_alloc(struct mtk_eth *
 		dma_addr_t dma_addr;
 		void *data;
 
-		rxd = ring->dma + i * eth->soc->txrx.rxd_size;
+		rxd = ring->dma + i * eth->soc->rx.desc_size;
 		if (ring->page_pool) {
 			data = mtk_page_pool_get_buff(ring->page_pool,
 						      &dma_addr, GFP_KERNEL);
@@ -2740,7 +2740,7 @@ static void mtk_rx_clean(struct mtk_eth
 			if (!ring->data[i])
 				continue;
 
-			rxd = ring->dma + i * eth->soc->txrx.rxd_size;
+			rxd = ring->dma + i * eth->soc->rx.desc_size;
 			if (!rxd->rxd1)
 				continue;
 
@@ -2757,7 +2757,7 @@ static void mtk_rx_clean(struct mtk_eth
 
 	if (!in_sram && ring->dma) {
 		dma_free_coherent(eth->dma_dev,
-				  ring->dma_size * eth->soc->txrx.rxd_size,
+				  ring->dma_size * eth->soc->rx.desc_size,
 				  ring->dma, ring->phys);
 		ring->dma = NULL;
 	}
@@ -3120,7 +3120,7 @@ static void mtk_dma_free(struct mtk_eth
 			netdev_reset_queue(eth->netdev[i]);
 	if (!MTK_HAS_CAPS(soc->caps, MTK_SRAM) && eth->scratch_ring) {
 		dma_free_coherent(eth->dma_dev,
-				  MTK_QDMA_RING_SIZE * soc->txrx.txd_size,
+				  MTK_QDMA_RING_SIZE * soc->tx.desc_size,
 				  eth->scratch_ring, eth->phy_scratch_ring);
 		eth->scratch_ring = NULL;
 		eth->phy_scratch_ring = 0;
@@ -3170,7 +3170,7 @@ static irqreturn_t mtk_handle_irq_rx(int
 
 	eth->rx_events++;
 	if (likely(napi_schedule_prep(&eth->rx_napi))) {
-		mtk_rx_irq_disable(eth, eth->soc->txrx.rx_irq_done_mask);
+		mtk_rx_irq_disable(eth, eth->soc->rx.irq_done_mask);
 		__napi_schedule(&eth->rx_napi);
 	}
 
@@ -3196,9 +3196,9 @@ static irqreturn_t mtk_handle_irq(int ir
 	const struct mtk_reg_map *reg_map = eth->soc->reg_map;
 
 	if (mtk_r32(eth, reg_map->pdma.irq_mask) &
-	    eth->soc->txrx.rx_irq_done_mask) {
+	    eth->soc->rx.irq_done_mask) {
 		if (mtk_r32(eth, reg_map->pdma.irq_status) &
-		    eth->soc->txrx.rx_irq_done_mask)
+		    eth->soc->rx.irq_done_mask)
 			mtk_handle_irq_rx(irq, _eth);
 	}
 	if (mtk_r32(eth, reg_map->tx_irq_mask) & MTK_TX_DONE_INT) {
@@ -3216,10 +3216,10 @@ static void mtk_poll_controller(struct n
 	struct mtk_eth *eth = mac->hw;
 
 	mtk_tx_irq_disable(eth, MTK_TX_DONE_INT);
-	mtk_rx_irq_disable(eth, eth->soc->txrx.rx_irq_done_mask);
+	mtk_rx_irq_disable(eth, eth->soc->rx.irq_done_mask);
 	mtk_handle_irq_rx(eth->irq[2], dev);
 	mtk_tx_irq_enable(eth, MTK_TX_DONE_INT);
-	mtk_rx_irq_enable(eth, eth->soc->txrx.rx_irq_done_mask);
+	mtk_rx_irq_enable(eth, eth->soc->rx.irq_done_mask);
 }
 #endif
 
@@ -3383,7 +3383,7 @@ static int mtk_open(struct net_device *d
 		napi_enable(&eth->tx_napi);
 		napi_enable(&eth->rx_napi);
 		mtk_tx_irq_enable(eth, MTK_TX_DONE_INT);
-		mtk_rx_irq_enable(eth, soc->txrx.rx_irq_done_mask);
+		mtk_rx_irq_enable(eth, soc->rx.irq_done_mask);
 		refcount_set(&eth->dma_refcnt, 1);
 	}
 	else
@@ -3467,7 +3467,7 @@ static int mtk_stop(struct net_device *d
 	mtk_gdm_config(eth, MTK_GDMA_DROP_ALL);
 
 	mtk_tx_irq_disable(eth, MTK_TX_DONE_INT);
-	mtk_rx_irq_disable(eth, eth->soc->txrx.rx_irq_done_mask);
+	mtk_rx_irq_disable(eth, eth->soc->rx.irq_done_mask);
 	napi_disable(&eth->tx_napi);
 	napi_disable(&eth->rx_napi);
 
@@ -3943,9 +3943,9 @@ static int mtk_hw_init(struct mtk_eth *e
 
 	/* FE int grouping */
 	mtk_w32(eth, MTK_TX_DONE_INT, reg_map->pdma.int_grp);
-	mtk_w32(eth, eth->soc->txrx.rx_irq_done_mask, reg_map->pdma.int_grp + 4);
+	mtk_w32(eth, eth->soc->rx.irq_done_mask, reg_map->pdma.int_grp + 4);
 	mtk_w32(eth, MTK_TX_DONE_INT, reg_map->qdma.int_grp);
-	mtk_w32(eth, eth->soc->txrx.rx_irq_done_mask, reg_map->qdma.int_grp + 4);
+	mtk_w32(eth, eth->soc->rx.irq_done_mask, reg_map->qdma.int_grp + 4);
 	mtk_w32(eth, 0x21021000, MTK_FE_INT_GRP);
 
 	if (mtk_is_netsys_v3_or_greater(eth)) {
@@ -5037,11 +5037,15 @@ static const struct mtk_soc_data mt2701_
 	.required_clks = MT7623_CLKS_BITMAP,
 	.required_pctl = true,
 	.version = 1,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
@@ -5057,11 +5061,15 @@ static const struct mtk_soc_data mt7621_
 	.offload_version = 1,
 	.hash_offset = 2,
 	.foe_entry_size = MTK_FOE_ENTRY_V1_SIZE,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
@@ -5079,11 +5087,15 @@ static const struct mtk_soc_data mt7622_
 	.hash_offset = 2,
 	.has_accounting = true,
 	.foe_entry_size = MTK_FOE_ENTRY_V1_SIZE,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
@@ -5100,11 +5112,15 @@ static const struct mtk_soc_data mt7623_
 	.hash_offset = 2,
 	.foe_entry_size = MTK_FOE_ENTRY_V1_SIZE,
 	.disable_pll_modes = true,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
@@ -5119,11 +5135,15 @@ static const struct mtk_soc_data mt7629_
 	.required_pctl = false,
 	.has_accounting = true,
 	.version = 1,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
@@ -5141,11 +5161,15 @@ static const struct mtk_soc_data mt7981_
 	.hash_offset = 4,
 	.has_accounting = true,
 	.foe_entry_size = MTK_FOE_ENTRY_V2_SIZE,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma_v2),
-		.rxd_size = sizeof(struct mtk_rx_dma_v2),
-		.rx_irq_done_mask = MTK_RX_DONE_INT_V2,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID_V2,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma_v2),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
+		.dma_len_offset = 8,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma_v2),
+		.irq_done_mask = MTK_RX_DONE_INT_V2,
+		.dma_l4_valid = RX_DMA_L4_VALID_V2,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
 		.dma_len_offset = 8,
 	},
@@ -5163,11 +5187,15 @@ static const struct mtk_soc_data mt7986_
 	.hash_offset = 4,
 	.has_accounting = true,
 	.foe_entry_size = MTK_FOE_ENTRY_V2_SIZE,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma_v2),
-		.rxd_size = sizeof(struct mtk_rx_dma_v2),
-		.rx_irq_done_mask = MTK_RX_DONE_INT_V2,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID_V2,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma_v2),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
+		.dma_len_offset = 8,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma_v2),
+		.irq_done_mask = MTK_RX_DONE_INT_V2,
+		.dma_l4_valid = RX_DMA_L4_VALID_V2,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
 		.dma_len_offset = 8,
 	},
@@ -5185,11 +5213,15 @@ static const struct mtk_soc_data mt7988_
 	.hash_offset = 4,
 	.has_accounting = true,
 	.foe_entry_size = MTK_FOE_ENTRY_V3_SIZE,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma_v2),
-		.rxd_size = sizeof(struct mtk_rx_dma_v2),
-		.rx_irq_done_mask = MTK_RX_DONE_INT_V2,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID_V2,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma_v2),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
+		.dma_len_offset = 8,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma_v2),
+		.irq_done_mask = MTK_RX_DONE_INT_V2,
+		.dma_l4_valid = RX_DMA_L4_VALID_V2,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
 		.dma_len_offset = 8,
 	},
@@ -5202,11 +5234,15 @@ static const struct mtk_soc_data rt5350_
 	.required_clks = MT7628_CLKS_BITMAP,
 	.required_pctl = false,
 	.version = 1,
-	.txrx = {
-		.txd_size = sizeof(struct mtk_tx_dma),
-		.rxd_size = sizeof(struct mtk_rx_dma),
-		.rx_irq_done_mask = MTK_RX_DONE_INT,
-		.rx_dma_l4_valid = RX_DMA_L4_VALID_PDMA,
+	.tx = {
+		.desc_size = sizeof(struct mtk_tx_dma),
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
+	},
+	.rx = {
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
+		.dma_l4_valid = RX_DMA_L4_VALID_PDMA,
 		.dma_max_len = MTK_TX_DMA_BUF_LEN,
 		.dma_len_offset = 16,
 	},
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -327,8 +327,8 @@
 /* QDMA descriptor txd3 */
 #define TX_DMA_OWNER_CPU	BIT(31)
 #define TX_DMA_LS0		BIT(30)
-#define TX_DMA_PLEN0(x)		(((x) & eth->soc->txrx.dma_max_len) << eth->soc->txrx.dma_len_offset)
-#define TX_DMA_PLEN1(x)		((x) & eth->soc->txrx.dma_max_len)
+#define TX_DMA_PLEN0(x)		(((x) & eth->soc->tx.dma_max_len) << eth->soc->tx.dma_len_offset)
+#define TX_DMA_PLEN1(x)		((x) & eth->soc->tx.dma_max_len)
 #define TX_DMA_SWC		BIT(14)
 #define TX_DMA_PQID		GENMASK(3, 0)
 #define TX_DMA_ADDR64_MASK	GENMASK(3, 0)
@@ -348,8 +348,8 @@
 /* QDMA descriptor rxd2 */
 #define RX_DMA_DONE		BIT(31)
 #define RX_DMA_LSO		BIT(30)
-#define RX_DMA_PREP_PLEN0(x)	(((x) & eth->soc->txrx.dma_max_len) << eth->soc->txrx.dma_len_offset)
-#define RX_DMA_GET_PLEN0(x)	(((x) >> eth->soc->txrx.dma_len_offset) & eth->soc->txrx.dma_max_len)
+#define RX_DMA_PREP_PLEN0(x)	(((x) & eth->soc->rx.dma_max_len) << eth->soc->rx.dma_len_offset)
+#define RX_DMA_GET_PLEN0(x)	(((x) >> eth->soc->rx.dma_len_offset) & eth->soc->rx.dma_max_len)
 #define RX_DMA_VTAG		BIT(15)
 #define RX_DMA_ADDR64_MASK	GENMASK(3, 0)
 #if IS_ENABLED(CONFIG_64BIT)
@@ -1153,10 +1153,9 @@ struct mtk_reg_map {
  * @foe_entry_size		Foe table entry size.
  * @has_accounting		Bool indicating support for accounting of
  *				offloaded flows.
- * @txd_size			Tx DMA descriptor size.
- * @rxd_size			Rx DMA descriptor size.
- * @rx_irq_done_mask		Rx irq done register mask.
- * @rx_dma_l4_valid		Rx DMA valid register mask.
+ * @desc_size			Tx/Rx DMA descriptor size.
+ * @irq_done_mask		Rx irq done register mask.
+ * @dma_l4_valid		Rx DMA valid register mask.
  * @dma_max_len			Max DMA tx/rx buffer length.
  * @dma_len_offset		Tx/Rx DMA length field offset.
  */
@@ -1174,13 +1173,17 @@ struct mtk_soc_data {
 	bool		has_accounting;
 	bool		disable_pll_modes;
 	struct {
-		u32	txd_size;
-		u32	rxd_size;
-		u32	rx_irq_done_mask;
-		u32	rx_dma_l4_valid;
+		u32	desc_size;
 		u32	dma_max_len;
 		u32	dma_len_offset;
-	} txrx;
+	} tx;
+	struct {
+		u32	desc_size;
+		u32	irq_done_mask;
+		u32	dma_l4_valid;
+		u32	dma_max_len;
+		u32	dma_len_offset;
+	} rx;
 };
 
 #define MTK_DMA_MONITOR_TIMEOUT		msecs_to_jiffies(1000)
