From patchwork Fri Apr 19 16:59:07 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 13636668
Return-Path: 
 <linux-mediatek-bounces+linux-mediatek=archiver.kernel.org@lists.infradead.org>
Date: Fri, 19 Apr 2024 17:59:07 +0100
From: Daniel Golle <daniel@makrotopia.org>
To: "Rafael J. Wysocki" <rafael@kernel.org>,
	Viresh Kumar <viresh.kumar@linaro.org>,
	Matthias Brugger <matthias.bgg@gmail.com>,
	AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>,
	linux-pm@vger.kernel.org, linux-kernel@vger.kernel.org,
	linux-arm-kernel@lists.infradead.org,
	linux-mediatek@lists.infradead.org
Subject: [PATCH] cpufreq: mediatek: Add support for MT7988A
Message-ID: 
 <acf4fb446aacfbf6ce7b6e94bf3aad303e0ad4d1.1713545923.git.daniel@makrotopia.org>
Content-Disposition: inline
List-Id: <linux-mediatek.lists.infradead.org>

From: Sam Shih <sam.shih@mediatek.com>

This add cpufreq support for mediatek MT7988A SoC.

The platform data of MT7988A is different from previous MediaTek SoCs,
so we add a new compatible and platform data for it.

Signed-off-by: Sam Shih <sam.shih@mediatek.com>
---
 drivers/cpufreq/mediatek-cpufreq.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/cpufreq/mediatek-cpufreq.c
+++ b/drivers/cpufreq/mediatek-cpufreq.c
@@ -707,6 +707,15 @@ static const struct mtk_cpufreq_platform
 	.ccifreq_supported = false,
 };
 
+static const struct mtk_cpufreq_platform_data mt7988_platform_data = {
+	.min_volt_shift = 100000,
+	.max_volt_shift = 200000,
+	.proc_max_volt = 900000,
+	.sram_min_volt = 0,
+	.sram_max_volt = 1150000,
+	.ccifreq_supported = true,
+};
+
 static const struct mtk_cpufreq_platform_data mt8183_platform_data = {
 	.min_volt_shift = 100000,
 	.max_volt_shift = 200000,
@@ -740,6 +749,8 @@ static const struct of_device_id mtk_cpu
 	{ .compatible = "mediatek,mt2712", .data = &mt2701_platform_data },
 	{ .compatible = "mediatek,mt7622", .data = &mt7622_platform_data },
 	{ .compatible = "mediatek,mt7623", .data = &mt7623_platform_data },
+	{ .compatible = "mediatek,mt7988a", .data = &mt7988_platform_data },
+	{ .compatible = "mediatek,mt7988d", .data = &mt7988_platform_data },
 	{ .compatible = "mediatek,mt8167", .data = &mt8516_platform_data },
 	{ .compatible = "mediatek,mt817x", .data = &mt2701_platform_data },
 	{ .compatible = "mediatek,mt8173", .data = &mt2701_platform_data },
