// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9342_ubnt_xw.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "ubnt,litebeam-m5-xw", "qca,ar9342";
	model = "Ubiquiti LiteBeam M5 (XW)";

	aliases {
		led-boot = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
		led-failsafe = &led_status;
		label-mac-device = &wmac;
	};

	leds {
		compatible = "gpio-leds";

		led-lan {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led-wlan {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			linux,default-trigger = "phy0tpt";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led_status: led-power {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
		phy-mode = "mii";
		reset-gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy1>;
};
