// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "ruckus,gd11", "qca,ar7161";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
		label-mac-device = &eth0;
	};

	keys: keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";
		dir-green {
			label = "green:dir";
			gpios = <&gpio 6 GPIO_ACTIVE_HIGH>;
		};

		opt-green {
			label = "green:opt";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		led_power_green: power-green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led_power_red: power-red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			panic-indicator;
		};

		wlan2g-green {
			label = "green:wlan2g";
			gpios = <&gpio 2 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0assoc";
		};

		wlan2g-yellow {
			label = "yellow:wlan2g";
			gpios = <&gpio 3 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g-green {
			label = "green:wlan5g";
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1assoc";
		};

		wlan5g-yellow {
			label = "yellow:wlan5g";
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		ruckus-himem@3ff0000 {
			/* Ruckus Himem area used to control
			 * redundant boot image selection
			 */
			compatible = "nvmem-rmem";
			reg = <0x3ff0000 0x10000>;
			no-map;
		};
	};

	beamforming-2g-spi {
		compatible = "spi-gpio";
		mosi-gpios = <&ath9k0 5 GPIO_ACTIVE_HIGH>;
		sck-gpios = <&ath9k0 6 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		beamforming_2g_gpio: beamforming-2g-gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			registers-number = <1>;
			spi-max-frequency = <24000000>;
			gpio-controller;
			#gpio-cells = <2>;
		};
	};

	beamforming-5g-spi {
		compatible = "spi-gpio";
		mosi-gpios = <&ath9k1 5 GPIO_ACTIVE_HIGH>;
		sck-gpios = <&ath9k1 6 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		beamforming_5g_gpio: beamforming-5g-gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			registers-number = <1>;
			spi-max-frequency = <24000000>;
			gpio-controller;
			#gpio-cells = <2>;
		};
	};
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@11,0 { /* 2.4 GHz */
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;
		nvmem-cells = <&macaddr_bdata_60>;
		nvmem-cell-names = "mac-address";
		#gpio-cells = <2>;
		gpio-controller;
	};

	ath9k1: wifi@12,0 { /* 5 GHz */
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;
		nvmem-cells = <&macaddr_bdata_76>;
		nvmem-cell-names = "mac-address";
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@1e {
		reg = <0x1e>;
	};
};

&eth0 {
	status = "okay";
	nvmem-cells = <&macaddr_bdata_66>;
	nvmem-cell-names = "mac-address";

	pll-data = <0x00110000 0x00001099 0x00991099>;
	phy-handle = <&phy0>;
	phy-mode = "rgmii-id";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <104000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x40000>;
				label = "u-boot";
				read-only;
			};

			/* On stock FW this encompasses rcks_wlan.main,
			 * rcks_wlan.bkup and datafs partitions
			 */
			partition@40000 {
				compatible = "openwrt,uimage", "denx,uimage";
				reg = <0x40000 0xf40000>;
				label = "firmware";
			};

			partition@f80000 {
				reg = <0xf80000 0x40000>;
				label = "u-boot-env";

				nvmem-layout {
					compatible = "u-boot,env";
				};
			};

			board_data: partition@fc0000 {
				reg = <0xfc0000 0x40000>;
				label = "board-data";
				read-only;
			};
		};
	};
};

&usb1 {
	status = "okay";
};

&usb2 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};
