From bc1c5829ecc698e41379f461f1fd7e8d600b879f Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Wed, 25 Jan 2023 12:38:37 +0100
Subject: [PATCH 0031/1085] drm/vc4: hvs: Initialize the dlist allocation list
 entry

The vc4_hvs_dlist_allocation structure has a list that we don't
initialize when we allocate a new instance.

This makes any call reading the list structure (such as list_empty) fail
with a NULL pointer dereference.

Let's make sure our list is always initialized.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_hvs.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_hvs.c
+++ b/drivers/gpu/drm/vc4/vc4_hvs.c
@@ -457,6 +457,8 @@ vc4_hvs_alloc_dlist_entry(struct vc4_hvs
 	if (!alloc)
 		return ERR_PTR(-ENOMEM);
 
+	INIT_LIST_HEAD(&alloc->node);
+
 	spin_lock_irqsave(&hvs->mm_lock, flags);
 	ret = drm_mm_insert_node(&hvs->dlist_mm, &alloc->mm_node,
 				 dlist_count);
