From 12c511cd31c2dc6bd96e4a89f7709d515aa8a76b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ar=C4=B1n=C3=A7=20=C3=9CNAL?= <arinc.unal@arinc9.com>
Date: Tue, 6 Feb 2024 01:08:03 +0300
Subject: [PATCH 13/30] net: dsa: mt7530: move XTAL check to mt7530_setup()
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The crystal frequency concerns the switch core. The frequency should be
checked when the switch is being set up so the driver can reject the
unsupported hardware earlier and without requiring port 6 to be used.

Move it to mt7530_setup(). Drop the unnecessary function printing.

Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Reviewed-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: Arınç ÜNAL <arinc.unal@arinc9.com>
Link: https://lore.kernel.org/r/20240206-for-netnext-mt7530-improvements-2-v5-2-d7d92a185cb1@arinc9.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/mt7530.c | 13 ++++++-------
 1 file changed, 6 insertions(+), 7 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -422,13 +422,6 @@ mt7530_pad_clk_setup(struct dsa_switch *
 
 	xtal = mt7530_read(priv, MT7530_MHWTRAP) & HWTRAP_XTAL_MASK;
 
-	if (xtal == HWTRAP_XTAL_20MHZ) {
-		dev_err(priv->dev,
-			"%s: MT7530 with a 20MHz XTAL is not supported!\n",
-			__func__);
-		return -EINVAL;
-	}
-
 	switch (interface) {
 	case PHY_INTERFACE_MODE_RGMII:
 		trgint = 0;
@@ -2458,6 +2451,12 @@ mt7530_setup(struct dsa_switch *ds)
 		return -ENODEV;
 	}
 
+	if ((val & HWTRAP_XTAL_MASK) == HWTRAP_XTAL_20MHZ) {
+		dev_err(priv->dev,
+			"MT7530 with a 20MHz XTAL is not supported!\n");
+		return -EINVAL;
+	}
+
 	/* Reset the switch through internal reset */
 	mt7530_write(priv, MT7530_SYS_CTRL,
 		     SYS_CTRL_PHY_RST | SYS_CTRL_SW_RST |
