From 2b6508e2bab01bc7dbd74d06f2ef4d22b48811c7 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Thu, 2 May 2019 13:22:53 -0700
Subject: [PATCH 0167/1085] drm/v3d: Clock V3D down when not in use.

My various attempts at re-enabling runtime PM have failed, so just
crank the clock down when V3D is idle to reduce power consumption.

Signed-off-by: Eric Anholt <eric@anholt.net>

drm/v3d: Plug dma_fence leak

The irq_fence and done_fence are given a reference that is never
released. The necessary dma_fence_put()s seem to have been
deleted in error in an earlier commit.

Fixes: 0b73676836b2 ("drm/v3d: Clock V3D down when not in use.")

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/gpu/drm/v3d/v3d_drv.c | 18 +++++++++++++
 drivers/gpu/drm/v3d/v3d_drv.h |  6 +++++
 drivers/gpu/drm/v3d/v3d_gem.c | 49 +++++++++++++++++++++++++++++++++++
 3 files changed, 73 insertions(+)

--- a/drivers/gpu/drm/v3d/v3d_drv.c
+++ b/drivers/gpu/drm/v3d/v3d_drv.c
@@ -256,6 +256,21 @@ static int v3d_platform_drm_probe(struct
 		}
 	}
 
+	v3d->clk = devm_clk_get(dev, NULL);
+	if (IS_ERR(v3d->clk)) {
+		if (ret != -EPROBE_DEFER)
+			dev_err(dev, "Failed to get clock\n");
+		goto dev_free;
+	}
+	v3d->clk_up_rate = clk_get_rate(v3d->clk);
+	/* For downclocking, drop it to the minimum frequency we can get from
+	 * the CPRMAN clock generator dividing off our parent.  The divider is
+	 * 4 bits, but ask for just higher than that so that rounding doesn't
+	 * make cprman reject our rate.
+	 */
+	v3d->clk_down_rate =
+		(clk_get_rate(clk_get_parent(v3d->clk)) / (1 << 4)) + 10000;
+
 	if (v3d->ver < 41) {
 		ret = map_regs(v3d, &v3d->gca_regs, "gca");
 		if (ret)
@@ -281,6 +296,9 @@ static int v3d_platform_drm_probe(struct
 	if (ret)
 		goto irq_disable;
 
+	ret = clk_set_rate(v3d->clk, v3d->clk_down_rate);
+	WARN_ON_ONCE(ret != 0);
+
 	return 0;
 
 irq_disable:
--- a/drivers/gpu/drm/v3d/v3d_drv.h
+++ b/drivers/gpu/drm/v3d/v3d_drv.h
@@ -76,6 +76,12 @@ struct v3d_dev {
 	void __iomem *bridge_regs;
 	void __iomem *gca_regs;
 	struct clk *clk;
+	struct delayed_work clk_down_work;
+	unsigned long clk_up_rate, clk_down_rate;
+	struct mutex clk_lock;
+	u32 clk_refcount;
+	bool clk_up;
+
 	struct reset_control *reset;
 
 	/* Virtual and DMA addresses of the single shared page table. */
--- a/drivers/gpu/drm/v3d/v3d_gem.c
+++ b/drivers/gpu/drm/v3d/v3d_gem.c
@@ -4,6 +4,7 @@
 #include <linux/device.h>
 #include <linux/dma-mapping.h>
 #include <linux/io.h>
+#include <linux/clk.h>
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/reset.h>
@@ -19,6 +20,47 @@
 #include "v3d_trace.h"
 
 static void
+v3d_clock_down_work(struct work_struct *work)
+{
+	struct v3d_dev *v3d =
+		container_of(work, struct v3d_dev, clk_down_work.work);
+	int ret;
+
+	ret = clk_set_rate(v3d->clk, v3d->clk_down_rate);
+	v3d->clk_up = false;
+	WARN_ON_ONCE(ret != 0);
+}
+
+static void
+v3d_clock_up_get(struct v3d_dev *v3d)
+{
+	mutex_lock(&v3d->clk_lock);
+	if (v3d->clk_refcount++ == 0) {
+		cancel_delayed_work_sync(&v3d->clk_down_work);
+		if (!v3d->clk_up)  {
+			int ret;
+
+			ret = clk_set_rate(v3d->clk, v3d->clk_up_rate);
+			WARN_ON_ONCE(ret != 0);
+			v3d->clk_up = true;
+		}
+	}
+	mutex_unlock(&v3d->clk_lock);
+}
+
+static void
+v3d_clock_up_put(struct v3d_dev *v3d)
+{
+	mutex_lock(&v3d->clk_lock);
+	if (--v3d->clk_refcount == 0) {
+		schedule_delayed_work(&v3d->clk_down_work,
+				      msecs_to_jiffies(100));
+	}
+	mutex_unlock(&v3d->clk_lock);
+}
+
+
+static void
 v3d_init_core(struct v3d_dev *v3d, int core)
 {
 	/* Set OVRTMUOUT, which means that the texture sampler uniform
@@ -318,6 +360,7 @@ static void
 v3d_job_free(struct kref *ref)
 {
 	struct v3d_job *job = container_of(ref, struct v3d_job, refcount);
+	struct v3d_dev *v3d = job->v3d;
 	int i;
 
 	if (job->bo) {
@@ -329,6 +372,8 @@ v3d_job_free(struct kref *ref)
 	dma_fence_put(job->irq_fence);
 	dma_fence_put(job->done_fence);
 
+	v3d_clock_up_put(v3d);
+
 	if (job->perfmon)
 		v3d_perfmon_put(job->perfmon);
 
@@ -448,6 +493,7 @@ v3d_job_init(struct v3d_dev *v3d, struct
 			goto fail_deps;
 	}
 
+	v3d_clock_up_get(v3d);
 	kref_init(&job->refcount);
 
 	return 0;
@@ -1031,6 +1077,9 @@ v3d_gem_init(struct drm_device *dev)
 	if (ret)
 		return ret;
 
+	mutex_init(&v3d->clk_lock);
+	INIT_DELAYED_WORK(&v3d->clk_down_work, v3d_clock_down_work);
+
 	/* Note: We don't allocate address 0.  Various bits of HW
 	 * treat 0 as special, such as the occlusion query counters
 	 * where 0 means "disabled".
