// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "confiabits,mt7621-v1", "mediatek,mt7621-soc";
	model = "Confiabits MT7621 v1";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	keys {
		compatible = "gpio-keys";

		button-wps {
			label = "wps";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		button-reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: led-power-green {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led-wan-red {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led-wlan5 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_5GHZ;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-wps {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WPS;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led-wlan24 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_2GHZ;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-wan-green {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "radio";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_radio_0: eeprom@0 {
						reg = <0x0 0x400>;
					};

					eeprom_radio_8000: eeprom@8000 {
						reg = <0x8000 0x4da8>;
					};

					macaddr_radio_4: macaddr@4 {
						reg = <0x4 0x6>;
					};

					macaddr_radio_8004: macaddr@8004 {
						reg = <0x8004 0x6>;
					};
				};
			};

			partition@50000 {
				label = "firmware";
				compatible = "denx,uimage";
				reg = <0x50000 0xfb0000>;
			};
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_radio_4>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_radio_4>;
	nvmem-cell-names = "mac-address";
};

&ethphy4 {
	/delete-property/ interrupts;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <2400000 2500000>;

		nvmem-cells = <&eeprom_radio_0>;
		nvmem-cell-names = "eeprom";
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <5000000 6000000>;

		nvmem-cells = <&eeprom_radio_8000>;
		nvmem-cell-names = "eeprom";
	};
};

&state_default {
	gpio {
		groups = "i2c", "jtag", "wdt";
		function = "gpio";
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan1";
		};

		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};
	};
};
