From 418603fdce51212d4547aacfe2b4801fc5e61978 Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <kernel@esmil.dk>
Date: Sat, 20 Nov 2021 21:33:08 +0100
Subject: [PATCH 1015/1024] RISC-V: Add StarFive JH7100 audio reset node

Add device tree node for the audio resets on the StarFive JH7100 RISC-V
SoC.

Signed-off-by: Emil Renner Berthing <kernel@esmil.dk>
---
 arch/riscv/boot/dts/starfive/jh7100.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/riscv/boot/dts/starfive/jh7100.dtsi
+++ b/arch/riscv/boot/dts/starfive/jh7100.dtsi
@@ -168,6 +168,12 @@
 			#clock-cells = <1>;
 		};
 
+		audrst: reset-controller@10490000 {
+			compatible = "starfive,jh7100-audrst";
+			reg = <0x0 0x10490000 0x0 0x10000>;
+			#reset-cells = <1>;
+		};
+
 		clkgen: clock-controller@11800000 {
 			compatible = "starfive,jh7100-clkgen";
 			reg = <0x0 0x11800000 0x0 0x10000>;
