From ad1915e2070cf832bfb81dcbeb44b073c09e6dcc Mon Sep 17 00:00:00 2001
From: Rosen Penev <rosenp@gmail.com>
Date: Sun, 20 Oct 2024 18:51:47 -0700
Subject: [PATCH] ARM: dts: meraki-mr26: set mac address for gmac0

Currently this needs to be done in userspace.

Signed-off-by: Rosen Penev <rosenp@gmail.com>
Link: https://lore.kernel.org/r/20241021015147.172700-1-rosenp@gmail.com
Signed-off-by: Florian Fainelli <florian.fainelli@broadcom.com>
---
 .../dts/broadcom/bcm53015-meraki-mr26.dts     | 20 +++++++++++++++++++
 1 file changed, 20 insertions(+)

--- a/arch/arm/boot/dts/broadcom/bcm53015-meraki-mr26.dts
+++ b/arch/arm/boot/dts/broadcom/bcm53015-meraki-mr26.dts
@@ -59,6 +59,9 @@
 
 &gmac0 {
 	status = "okay";
+
+	nvmem-cells = <&macaddr_board_config_66>;
+	nvmem-cell-names = "mac-address";
 };
 
 &gmac1 {
@@ -102,8 +105,25 @@
 		};
 
 		partition@800000 {
+			compatible = "linux,ubi";
 			label = "ubi";
 			reg = <0x800000 0x7780000>;
+
+			volumes {
+				ubi-volume-board-config {
+					volname = "board-config";
+
+					nvmem-layout {
+						compatible = "fixed-layout";
+						#address-cells = <1>;
+						#size-cells = <1>;
+
+						macaddr_board_config_66: macaddr@66 {
+							reg = <0x66 0x6>;
+						};
+					};
+				};
+			};
 		};
 	};
 };
