--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -416,6 +416,12 @@ config ROCKCHIP_PHY
 	help
 	  Currently supports the integrated Ethernet PHY.
 
+config RTL8367S_GSW
+	tristate "rtl8367 Gigabit Switch support for mt7622"
+	depends on NET_VENDOR_MEDIATEK
+	help
+	  This driver supports rtl8367s in mt7622
+
 config SMSC_PHY
 	tristate "SMSC PHYs"
 	select CRC16
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -102,6 +102,7 @@ obj-$(CONFIG_QSEMI_PHY)		+= qsemi.o
 obj-$(CONFIG_REALTEK_PHY)	+= realtek/
 obj-$(CONFIG_RENESAS_PHY)	+= uPD60620.o
 obj-$(CONFIG_ROCKCHIP_PHY)	+= rockchip.o
+obj-$(CONFIG_RTL8367S_GSW)	+= rtk/
 obj-$(CONFIG_SMSC_PHY)		+= smsc.o
 obj-$(CONFIG_STE10XP)		+= ste10Xp.o
 obj-$(CONFIG_TERANETICS_PHY)	+= teranetics.o
