From e04a5456fd53dddcff0d33c0c6647270c2f5fbf7 Mon Sep 17 00:00:00 2001
From: Jonathan Lemon <jonathan.lemon@gmail.com>
Date: Wed, 4 May 2022 14:33:05 -0700
Subject: [PATCH 0382/1085] Populate phy driver block for BCM54213PE

The BCM54213PE identifier is a RPI-specific addition.
Populate the remainder of the driver functions, including the
required probe routine.

Add a version of bcm54xx_suspend, from upstream.

Signed-off-by: Jonathan Lemon <jonathan.lemon@gmail.com>
---
 drivers/net/phy/broadcom.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/net/phy/broadcom.c
+++ b/drivers/net/phy/broadcom.c
@@ -1050,8 +1050,14 @@ static struct phy_driver broadcom_driver
 	.phy_id_mask	= 0xffffffff,
 	.name		= "Broadcom BCM54213PE",
 	/* PHY_GBIT_FEATURES */
+	.get_sset_count	= bcm_phy_get_sset_count,
+	.get_strings	= bcm_phy_get_strings,
+	.get_stats	= bcm54xx_get_stats,
+	.probe		= bcm54xx_phy_probe,
 	.config_init	= bcm54xx_config_init,
 	.config_intr	= bcm_phy_config_intr,
+	.suspend	= bcm54xx_suspend,
+	.resume		= bcm54xx_resume,
 }, {
 	.phy_id		= PHY_ID_BCM5461,
 	.phy_id_mask	= 0xfffffff0,
