--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -40,6 +40,17 @@ config BSC9132_QDS
 	  and dual StarCore SC3850 DSP cores.
 	  Manufacturer : Freescale Semiconductor, Inc
 
+config HIVEAP_330
+    bool "Aerohive HiveAP-330"
+    select DEFAULT_UIMAGE
+    select ARCH_REQUIRE_GPIOLIB
+    select GPIO_MPC8XXX
+    help
+      This option enables support for the Aerohive HiveAP-330 board.
+
+      This board is a Concurrent Dual-Band wireless access point with a
+      Freescale P1020 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -12,6 +12,7 @@ obj-y += common.o
 obj-$(CONFIG_BSC9131_RDB) += bsc913x_rdb.o
 obj-$(CONFIG_BSC9132_QDS) += bsc913x_qds.o
 obj-$(CONFIG_C293_PCIE)   += c293pcie.o
+obj-$(CONFIG_HIVEAP_330) += hiveap-330.o
 obj-$(CONFIG_MPC8536_DS)  += mpc8536_ds.o
 obj8259-$(CONFIG_PPC_I8259)   += mpc85xx_8259.o
 obj-$(CONFIG_MPC85xx_DS)  += mpc85xx_ds.o $(obj8259-y)
--- a/arch/powerpc/boot/Makefile
+++ b/arch/powerpc/boot/Makefile
@@ -182,6 +182,7 @@ src-plat-$(CONFIG_PPC_PSERIES) += pserie
 src-plat-$(CONFIG_PPC_POWERNV) += pseries-head.S
 src-plat-$(CONFIG_PPC_IBM_CELL_BLADE) += pseries-head.S
 src-plat-$(CONFIG_MVME7100) += motload-head.S mvme7100.c
+src-plat-$(CONFIG_HIVEAP_330) += simpleboot.c fixed-head.S
 src-plat-$(CONFIG_TL_WDR4900_V1) += simpleboot.c fixed-head.S
 
 src-plat-$(CONFIG_PPC_MICROWATT) += fixed-head.S microwatt.c
@@ -354,6 +355,7 @@ image-$(CONFIG_TQM8548)			+= cuImage.tqm
 image-$(CONFIG_TQM8555)			+= cuImage.tqm8555
 image-$(CONFIG_TQM8560)			+= cuImage.tqm8560
 image-$(CONFIG_KSI8560)			+= cuImage.ksi8560
+image-$(CONFIG_HIVEAP_330)		+= simpleImage.hiveap-330
 image-$(CONFIG_TL_WDR4900_V1)		+= simpleImage.tl-wdr4900-v1
 # Board ports in arch/powerpc/platform/86xx/Kconfig
 image-$(CONFIG_MVME7100)                += dtbImage.mvme7100
--- a/arch/powerpc/boot/wrapper
+++ b/arch/powerpc/boot/wrapper
@@ -350,6 +350,7 @@ adder875-redboot)
     platformo="$object/fixed-head.o $object/redboot-8xx.o"
     binary=y
     ;;
+simpleboot-hiveap-330|\
 simpleboot-tl-wdr4900-v1)
     platformo="$object/fixed-head.o $object/simpleboot.o"
     link_address='0x1500000'
