// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	compatible = "skspruce,wia3300-20", "qcom,ipq4019";
	model = "SKSpruce WIA3300-20";

	aliases {
		// TODO: Verify if the ethernet0 alias is needed
		ethernet0 = &gmac;
		label-mac-device = &gmac;
		led-boot = &led_status_red;
		led-failsafe = &led_status_lime;
		led-running = &led_status_lime;
		led-upgrade = &led_status_red;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys";

		pinctrl-0 = <&key_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		led_status_red: led-0 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 8 GPIO_ACTIVE_LOW>;
		};

		led_status_lime: led-1 {
			color = <LED_COLOR_ID_LIME>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 9 GPIO_ACTIVE_LOW>;
		};

		led-2 {
			color = <LED_COLOR_ID_LIME>;
			function = LED_FUNCTION_WLAN_2GHZ;
			gpios = <&tlmm 11 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-3 {
			color = <LED_COLOR_ID_LIME>;
			function = LED_FUNCTION_WLAN_5GHZ;
			gpios = <&tlmm 28 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	output-usb-power {
		compatible = "regulator-output";
		vout-supply = <&reg_usb>;
	};

	reg_usb: regulator-usb {
		compatible = "regulator-fixed";

		pinctrl-0 = <&reg_usb_pins>;
		pinctrl-names = "default";

		enable-active-high;
		gpios = <&tlmm 25 GPIO_ACTIVE_HIGH>;
		regulator-max-microvolt = <5000000>;
		regulator-min-microvolt = <5000000>;
		regulator-name = "reg_usb";
		regulator-boot-on;
	};

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	status = "okay";

	pinctrl-0 = <&spi0_pins>;
	pinctrl-names = "default";

	cs-gpios = <&tlmm 12 GPIO_ACTIVE_LOW>;

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <24000000>;
		reg = <0>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};

			partition@40000 {
				label = "0:MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};

			partition@60000 {
				label = "0:QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};

			partition@c0000 {
				label = "0:CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};

			partition@d0000 {
				label = "0:DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};

			partition@e0000 {
				compatible = "u-boot,env";
				label = "0:APPSBLENV";
				reg = <0x000e0000 0x00010000>;
			};

			partition@f0000 {
				label = "0:APPSBL";
				reg = <0x000f0000 0x00080000>;
				read-only;
			};

			partition@170000 {
				label = "0:oldART";
				reg = <0x00170000 0x00010000>;
				read-only;
			};

			partition@180000 {
				label = "0:HLOS";
				reg = <0x00180000 0x00800000>;
				read-only;
			};

			partition@980000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x980000 0x35d0000>;
			};

			partition@3f50000 {
				label = "0:APPSBL1";
				reg = <0x03f50000 0x00080000>;
				read-only;
			};

			partition@3fd0000 {
				label = "BoardInfo";
				reg = <0x03fd0000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_boardinfo_108a: macaddr@108a {
						compatible = "mac-base";
						reg = <0x108a 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@3fe0000 {
				label = "RebootCause";
				reg = <0x03fe0000 0x00010000>;
				read-only;
			};

			partition@3ff0000 {
				label = "0:ART";
				reg = <0x03ff0000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};

&blsp1_uart1 {
	status = "okay";

	pinctrl-0 = <&serial0_pins>;
	pinctrl-names = "default";
};

&crypto {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&ethphy3 {
	leds {
		#address-cells = <1>;
		#size-cells = <0>;

		led@1 {
			reg = <1>;
			color = <LED_COLOR_ID_LIME>;
			function = LED_FUNCTION_LAN;
		};
	};
};

&ethphy4 {
	leds {
		#address-cells = <1>;
		#size-cells = <0>;

		led@1 {
			reg = <1>;
			color = <LED_COLOR_ID_LIME>;
			function = LED_FUNCTION_WAN;
		};
	};
};

&gmac {
	status = "okay";

	nvmem-cells = <&macaddr_boardinfo_108a 0>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	status = "okay";

	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";

	reset-delay-us = <2000>;
	reset-post-delay-us = <2000>;
	reset-gpios = <&tlmm 43 GPIO_ACTIVE_LOW>;
};

&prng {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";

	label = "ETH2";
	nvmem-cells = <&macaddr_boardinfo_108a 1>;
	nvmem-cell-names = "mac-address";
};

&swport5 {
	status = "okay";

	label = "ETH1";
	nvmem-cells = <&macaddr_boardinfo_108a 0>;
	nvmem-cell-names = "mac-address";
};

&tlmm {
	key_pins: key_pinmux {
		gpio {
			pins = "gpio18";
			function = "gpio";
			bias-disable;
		};
	};

	led_pins: led_pinmux {
		gpio {
			pins = "gpio8", "gpio9", "gpio11", "gpio28";
			function = "gpio";
			drive-strength = <8>;
			drive-open-drain;
			bias-disable;
		};
	};

	mdio_pins: mdio_pinmux {
		gpio {
			pins = "gpio43";
			function = "gpio";
			drive-strength = <4>;
			bias-disable;
			output-high;
		};

		mdc {
			pins = "gpio7";
			function = "mdc";
			drive-strength = <4>;
			bias-disable;
		};

		mdio {
			pins = "gpio6";
			function = "mdio";
			drive-strength = <4>;
			drive-open-drain;
			bias-pull-up;
		};
	};

	reg_usb_pins: reg_usb_pinmux {
		gpio {
			pins = "gpio25";
			function = "gpio";
			drive-strength = <8>;
			bias-disable;
			output-high;
		};
	};

	serial0_pins: serial0_pinmux {
		blsp_uart0 {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			drive-strength = <8>;
			bias-disable;
		};
	};

	spi0_pins: spi0_pinmux {
		blsp_spi0 {
			pins = "gpio13", "gpio14", "gpio15";
			function = "blsp_spi0";
			drive-strength = <4>;
			bias-disable;
		};

		gpio {
			pins = "gpio12";
			function = "gpio";
			drive-strength = <4>;
			bias-disable;
			output-high;
		};
	};
};

&usb2 {
	status = "okay";
};

&usb2_hs_phy {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&wifi0 {
	status = "okay";

	nvmem-cell-names = "mac-address", "pre-calibration";
	nvmem-cells = <&macaddr_boardinfo_108a 3>, <&precal_art_1000>;
	qcom,ath10k-calibration-variant = "SKSpruce_WIA3300-20";
};

&wifi1 {
	status = "okay";

	nvmem-cell-names = "mac-address", "pre-calibration";
	nvmem-cells = <&macaddr_boardinfo_108a 4>, <&precal_art_5000>;
	qcom,ath10k-calibration-variant = "SKSpruce_WIA3300-20";
};
