#!/bin/sh

[ -e /lib/firmware/$FIRMWARE ] && exit 0

. /lib/functions/caldata.sh

board=$(board_name)

case "$FIRMWARE" in
"ath9k-eeprom-ahb-18100000.wmac.bin")
	case $board in
	asus,pl-ac56|\
	asus,rp-ac51|\
	asus,rp-ac66)
		caldata_extract "art" 0x1000 0x440
		;;
	avm,fritz1750e|\
	avm,fritz4020|\
	avm,fritz450e|\
	avm,fritzdvbc)
		caldata_extract_reverse "urlader" 0x1541 0x440
		;;
	dlink,dir-505)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_text "mac" 0x4)
		;;
	dlink,dir-842-c1|\
	dlink,dir-842-c2|\
	dlink,dir-842-c3|\
	wd,mynet-n600|\
	wd,mynet-n750)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii devdata "wlan24mac")
		;;
	engenius,ecb1200|\
	engenius,ecb1750)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(macaddr_add $(mtd_get_mac_ascii u-boot-env athaddr) 1)
		;;
	enterasys,ws-ap3705i)
		caldata_extract "calibrate" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii u-boot-env0 RADIOADDR1)
		;;
	extreme-networks,ws-ap3805i)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii cfg1 RADIOADDR1)
		;;
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr|\
	sitecom,wlr-7100|\
	sitecom,wlr-8100)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii u-boot-env ethaddr)
		;;
	moxa,awk-1137c)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii u-boot-env mac_addr)
		;;
	*)
		caldata_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:00.0.bin")
	case $board in
	avm,fritz300e)
		caldata_extract_reverse "urloader" 0x1541 0x440
		;;
	buffalo,wzr-hp-g450h)
		caldata_extract "art" 0x1000 0x440
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1)
		caldata_extract "art" 0x5000 0x440
		ath9k_patch_mac $(macaddr_add $(mtd_get_mac_text "mac" 0x18) 1)
		;;
	enterasys,ws-ap3705i)
		caldata_extract "calibrate" 0x5000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii u-boot-env0 RADIOADDR0)
		;;
	meraki,mr12)
		caldata_extract "art" 0x11000 0xeb8
		;;
	ubnt,powerbridge-m|\
	ubnt,rocket-m)
		caldata_extract "art" 0x1000 0x1000
		;;
	wd,mynet-n600|\
	wd,mynet-n750)
		caldata_extract "art" 0x5000 0x440
		ath9k_patch_mac $(mtd_get_mac_ascii devdata "wlan5mac")
		;;
	wd,mynet-wifi-rangeextender)
		caldata_extract "art" 0x1000 0x440
		ath9k_patch_mac $(nvram get wl0_hwaddr)
		;;
	*)
		caldata_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:11.0.bin")
	case $board in
	buffalo,wzr-600dhp|\
	buffalo,wzr-hp-ag300h)
		caldata_extract "art" 0x1000 0xeb8
		;;
	trendnet,tew-673gru)
		caldata_extract "caldata" 0x1000 0xeb8
		ath9k_patch_mac_crc $(mtd_get_mac_text "caldata" 0xffa0) 0x20c
		;;
	meraki,mr16)
		caldata_extract "art" 0x11000 0xeb8
		;;
	*)
		caldata_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:12.0.bin")
	case $board in
	buffalo,wzr-600dhp|\
	buffalo,wzr-hp-ag300h)
		caldata_extract "art" 0x5000 0xeb8
		;;
	trendnet,tew-673gru)
		caldata_extract "caldata" 0x5000 0xeb8
		ath9k_patch_mac_crc $(macaddr_add $(mtd_get_mac_text "caldata" 0xffb4) 1) 0x20c
		;;
	meraki,mr16)
		caldata_extract "art" 0x15000 0xeb8
		;;
	*)
		caldata_die "board $board is not supported yet"
		;;
	esac
	;;
esac
