From 3a8b7204348682152b77618eed061e8718db5935 Mon Sep 17 00:00:00 2001
From: Stefan Wahren <stefan.wahren@chargebyte.com>
Date: Wed, 1 May 2024 11:18:49 +0200
Subject: [PATCH 1075/1085] overlays: qca7000: Adjust URL & README info

in-tech smart charging is now called chargebyte. Our product name
seems to be more stable than our company name, so drop them
where it's possible.

Signed-off-by: Stefan Wahren <stefan.wahren@chargebyte.com>
---
 arch/arm/boot/dts/overlays/README              | 4 ++--
 arch/arm/boot/dts/overlays/qca7000-overlay.dts | 2 +-
 2 files changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -3844,7 +3844,7 @@ Params: clock                   PWM cloc
 
 
 Name:   qca7000
-Info:   in-tech's Evaluation Board for PLC Stamp micro
+Info:   Evaluation Board for PLC Stamp micro
         This uses spi0 and a separate GPIO interrupt to connect the QCA7000.
 Load:   dtoverlay=qca7000,<param>=<val>
 Params: int_pin                 GPIO pin for interrupt signal (default 23)
@@ -3853,7 +3853,7 @@ Params: int_pin                 GPIO pin
 
 
 Name:   qca7000-uart0
-Info:   in-tech's Evaluation Board for PLC Stamp micro (UART)
+Info:   Evaluation Board for PLC Stamp micro (UART)
         This uses uart0/ttyAMA0 over GPIOs 14 & 15 to connect the QCA7000.
         But it requires disabling of onboard Bluetooth on
         Pi 3B, 3B+, 3A+, 4B and Zero W.
--- a/arch/arm/boot/dts/overlays/qca7000-overlay.dts
+++ b/arch/arm/boot/dts/overlays/qca7000-overlay.dts
@@ -1,5 +1,5 @@
 // Overlay for the Qualcomm Atheros QCA7000 on PLC Stamp micro EVK
-// Visit: https://in-tech-smartcharging.com/products/evaluation-tools/plc-stamp-micro-2-evaluation-board for details
+// Visit: https://chargebyte.com/products/evaluation-tools/plc-stamp-micro-2-evaluation-board for details
 
 /dts-v1/;
 /plugin/;
