From 400909df6e6543cb5cce3db9bbcd413d59125327 Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Sat, 10 Feb 2024 17:58:29 +0100
Subject: [PATCH] r8169: simplify code by using core-provided pcpu stats
 allocation

Use core-provided pcpu stats allocation instead of open-coding it in
the driver.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Link: https://lore.kernel.org/r/03f5bb3b-d7f4-48be-ae8a-54862ec4566c@gmail.com
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/ethernet/realtek/r8169_main.c | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -5296,11 +5296,6 @@ static int rtl_init_one(struct pci_dev *
 	raw_spin_lock_init(&tp->mac_ocp_lock);
 	mutex_init(&tp->led_lock);
 
-	dev->tstats = devm_netdev_alloc_pcpu_stats(&pdev->dev,
-						   struct pcpu_sw_netstats);
-	if (!dev->tstats)
-		return -ENOMEM;
-
 	/* Get the *optional* external "ether_clk" used on some boards */
 	tp->clk = devm_clk_get_optional_enabled(&pdev->dev, "ether_clk");
 	if (IS_ERR(tp->clk))
@@ -5415,6 +5410,8 @@ static int rtl_init_one(struct pci_dev *
 	dev->hw_features |= NETIF_F_RXALL;
 	dev->hw_features |= NETIF_F_RXFCS;
 
+	dev->pcpu_stat_type = NETDEV_PCPU_STAT_TSTATS;
+
 	netdev_sw_irq_coalesce_default_on(dev);
 
 	/* configure chip for default features */
