From f5ebf9ab60940b00c36dfe64add41c80f3daff6a Mon Sep 17 00:00:00 2001
From: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Date: Tue, 11 Jun 2024 15:54:27 +0200
Subject: net: dsa: lantiq_gswip: Don't manually call gswip_port_enable()

We don't need to manually call gswip_port_enable() from within
gswip_setup() for the CPU port. DSA does this automatically for us.

Signed-off-by: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Acked-by: Hauke Mehrtens <hauke@hauke-m.de>
Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Signed-off-by: Martin Schiller <ms@dev.tdt.de>
Link: https://lore.kernel.org/r/20240611135434.3180973-6-ms@dev.tdt.de
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/lantiq_gswip.c | 2 --
 1 file changed, 2 deletions(-)

--- a/drivers/net/dsa/lantiq_gswip.c
+++ b/drivers/net/dsa/lantiq_gswip.c
@@ -891,8 +891,6 @@ static int gswip_setup(struct dsa_switch
 
 	ds->mtu_enforcement_ingress = true;
 
-	gswip_port_enable(ds, cpu_port, NULL);
-
 	ds->configure_vlan_while_not_filtering = false;
 
 	return 0;
