From 0dc3500c06a5d2d888a4afb648ded127a8639515 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 16 Mar 2022 12:15:41 +0000
Subject: [PATCH 0356/1085] media: i2c: ov5647: Use
 v4l2_async_register_subdev_sensor for lens binding

v4l2_async_register_subdev doesn't bind in lens or flash drivers,
but v4l2_async_register_subdev_sensor does.
Switch to using v4l2_async_register_subdev_sensor.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/i2c/ov5647.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -1575,7 +1575,7 @@ static int ov5647_probe(struct i2c_clien
 	if (ret < 0)
 		goto power_off;
 
-	ret = v4l2_async_register_subdev(sd);
+	ret = v4l2_async_register_subdev_sensor(sd);
 	if (ret < 0)
 		goto power_off;
 
