From f1bbbb260a8016373adf239c716d2da90e6ced0b Mon Sep 17 00:00:00 2001
From: Hayes Wang <hayeswang@realtek.com>
Date: Fri, 16 Apr 2021 16:04:32 +0800
Subject: [PATCH] r8152: set inter fram gap time depending on speed

commit 5133bcc7481528e36fff0a3b056601efb704fb32 upstream.

Set the maximum inter frame gap time (144ns) for speed 10M/half and
100M/half. It improves the performance for those speeds. And, there
is no effect for the other speeds.

For 10M/half and 100M/half, the fast inter frame gap time let the
device couldn't use the feature of the aggregation effectively,
because the transfer would be completed fastly. Therefore, use the
maximum value to improve the effect of the aggregation. However, you
may not feel the improvement for fast CPUs, because they compensate
for the effect of the aggregation.

Signed-off-by: Hayes Wang <hayeswang@realtek.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/r8152.c | 28 ++++++++++++++++++++++++++++
 1 file changed, 28 insertions(+)

--- a/drivers/net/usb/r8152.c
+++ b/drivers/net/usb/r8152.c
@@ -250,6 +250,9 @@
 
 /* PLA_TCR1 */
 #define VERSION_MASK		0x7cf0
+#define IFG_MASK		(BIT(3) | BIT(9) | BIT(8))
+#define IFG_144NS		BIT(9)
+#define IFG_96NS		(BIT(9) | BIT(8))
 
 /* PLA_MTPS */
 #define MTPS_JUMBO		(12 * 1024 / 64)
@@ -2748,6 +2751,29 @@ static int rtl_stop_rx(struct r8152 *tp)
 	return 0;
 }
 
+static void rtl_set_ifg(struct r8152 *tp, u16 speed)
+{
+	u32 ocp_data;
+
+	ocp_data = ocp_read_word(tp, MCU_TYPE_PLA, PLA_TCR1);
+	ocp_data &= ~IFG_MASK;
+	if ((speed & (_10bps | _100bps)) && !(speed & FULL_DUP)) {
+		ocp_data |= IFG_144NS;
+		ocp_write_word(tp, MCU_TYPE_PLA, PLA_TCR1, ocp_data);
+
+		ocp_data = ocp_read_word(tp, MCU_TYPE_PLA, PLA_MAC_PWR_CTRL4);
+		ocp_data &= ~TX10MIDLE_EN;
+		ocp_write_word(tp, MCU_TYPE_PLA, PLA_MAC_PWR_CTRL4, ocp_data);
+	} else {
+		ocp_data |= IFG_96NS;
+		ocp_write_word(tp, MCU_TYPE_PLA, PLA_TCR1, ocp_data);
+
+		ocp_data = ocp_read_word(tp, MCU_TYPE_PLA, PLA_MAC_PWR_CTRL4);
+		ocp_data |= TX10MIDLE_EN;
+		ocp_write_word(tp, MCU_TYPE_PLA, PLA_MAC_PWR_CTRL4, ocp_data);
+	}
+}
+
 static inline void r8153b_rx_agg_chg_indicate(struct r8152 *tp)
 {
 	ocp_write_byte(tp, MCU_TYPE_USB, USB_UPT_RXDMA_OWN,
@@ -2851,6 +2877,8 @@ static int rtl8153_enable(struct r8152 *
 	r8153_set_rx_early_timeout(tp);
 	r8153_set_rx_early_size(tp);
 
+	rtl_set_ifg(tp, rtl8152_get_speed(tp));
+
 	if (tp->version == RTL_VER_09) {
 		u32 ocp_data;
 
