From 8fb908fe3f80d6bbc0a7f5e7fe14ababe7f87f83 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Mon, 11 Jan 2021 15:23:06 +0100
Subject: [PATCH] drm/vc4: hdmi: Don't register the CEC adapter if
 there's no interrupts

We introduced the BCM2711 support to the vc4 HDMI controller with 5.10,
but this was lacking any of the interrupts of the CEC controller so we
have to deal with the backward compatibility.

Do so by simply ignoring the CEC setup if the DT doesn't have the
interrupts property.

Reviewed-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_hdmi.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_hdmi.c
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.c
@@ -1787,9 +1787,15 @@ static int vc4_hdmi_cec_init(struct vc4_
 {
 	struct cec_connector_info conn_info;
 	struct platform_device *pdev = vc4_hdmi->pdev;
+	struct device *dev = &pdev->dev;
 	u32 value;
 	int ret;
 
+	if (!of_find_property(dev->of_node, "interrupts", NULL)) {
+		dev_warn(dev, "'interrupts' DT property is missing, no CEC\n");
+		return 0;
+	}
+
 	vc4_hdmi->cec_adap = cec_allocate_adapter(&vc4_hdmi_cec_adap_ops,
 						  vc4_hdmi, "vc4",
 						  CEC_CAP_DEFAULTS |
