// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6318.dtsi"

/ {
	model = "Comtrend AR-5315u";
	compatible = "comtrend,ar-5315u", "brcm,bcm6318";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;

		led-dsl = &led_dsl_green;
		led-internet = &led_internet_green;
		led-usb = &led_usb_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&pinctrl 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 33 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	bcm43217-sprom {
		compatible = "brcm,bcm43217-sprom";

		pci-bus = <1>;
		pci-dev = <0>;

		nvmem-cells = <&macaddr_cfe_6a0>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;

		brcm,sprom-fixups = <6 0x1c00>,
				    <65 0x1255>,
				    <97 0xfe55>,
				    <98 0x171d>,
				    <99 0xfa42>,
				    <113 0xfeb7>,
				    <114 0x18cd>,
				    <115 0xfa4f>,
				    <162 0x6444>,
				    <170 0x6444>,
				    <172 0x6444>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0>;
	nvmem-cell-names = "mac-address";
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <62500000>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			cfe: partition@0 {
				reg = <0x000000 0x010000>;
				label = "cfe";
				read-only;
			};

			partition@10000 {
				compatible = "brcm,bcm963xx-imagetag";
				reg = <0x010000 0xfe0000>;
				label = "firmware";
			};

			partition@ff0000 {
				reg = <0xff0000 0x010000>;
				label = "nvram";
			};
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds
		     &pinctrl_ephy0_act_led &pinctrl_ephy1_act_led
		     &pinctrl_ephy2_act_led &pinctrl_ephy3_act_led>;

	led@0 {
		reg = <0>;
		active-low;
		label = "green:wps";
	};

	led_power_green: led@1 {
		reg = <1>;
		active-low;
		label = "green:power";
	};

	led_usb_green: led@2 {
		reg = <2>;
		active-low;
		label = "green:usb";
	};

	led@4 {
		reg = <4>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <4>;
		/* EPHY0 Act */
	};

	led@5 {
		reg = <5>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <5>;
		/* EPHY1 Act */
	};

	led@6 {
		reg = <6>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <6>;
		/* EPHY2 Act */
	};

	led@7 {
		reg = <7>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <7>;
		/* EPHY3 Act */
	};

	led_internet_green: led@8 {
		reg = <8>;
		active-low;
		label = "green:internet";
	};

	led@9 {
		reg = <9>;
		active-low;
		label = "red:internet";
	};

	led_dsl_green: led@10 {
		reg = <10>;
		active-low;
		label = "green:dsl";
	};

	led_power_red: led@11 {
		reg = <11>;
		active-low;
		label = "red:power";
	};
};

&ohci {
	status = "okay";
};

&pcie {
	status = "okay";
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio0", "gpio1",
		       "gpio2", "gpio8",
		       "gpio9", "gpio10",
		       "gpio11";
	};
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "lan4";

			phy-handle = <&phy1>;
		};

		port@1 {
			reg = <1>;
			label = "lan3";

			phy-handle = <&phy2>;
		};

		port@2 {
			reg = <2>;
			label = "lan2";

			phy-handle = <&phy3>;
		};

		port@3 {
			reg = <3>;
			label = "lan1";

			phy-handle = <&phy4>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};

&cfe {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_cfe_6a0: macaddr@6a0 {
		reg = <0x6a0 0x6>;
	};
};
