From d0ae9c944b9472c5691a482297df7a57d7fd1199 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 19 Aug 2021 14:11:08 +0200
Subject: [PATCH] arm64: dts: broadcom: bcm4908: Fix NAND node name
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This matches nand-controller.yaml requirements.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
@@ -296,7 +296,7 @@
 			status = "okay";
 		};
 
-		nand@1800 {
+		nand-controller@1800 {
 			#address-cells = <1>;
 			#size-cells = <0>;
 			compatible = "brcm,nand-bcm63138", "brcm,brcmnand-v7.1", "brcm,brcmnand";
