From 9d276da259cce20b2ed7a868b6e6a6a205f7bb04 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 23 Sep 2021 19:20:13 +0200
Subject: [PATCH] phy: marvell: phy-mvebu-a3700-comphy: Add native kernel
 implementation
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Remove old RPC implementation and add a new native kernel implementation.

The old implementation uses ARM SMC API to issue RPC calls to ARM Trusted
Firmware which provides real implementation of PHY configuration.

But older versions of ARM Trusted Firmware do not provide this PHY
configuration functionality, simply returning: operation not supported; or
worse, some versions provide the configuration functionality incorrectly.

For example the firmware shipped in ESPRESSObin board has this older
version of ARM Trusted Firmware and therefore SATA, USB 3.0 and PCIe
functionality do not work with newer versions of Linux kernel.

Due to the above reasons, the following commits were introduced into Linux,
to workaround these issues by ignoring -EOPNOTSUPP error code from
phy-mvebu-a3700-comphy driver function phy_power_on():

commit 45aefe3d2251 ("ata: ahci: mvebu: Make SATA PHY optional for Armada
3720")
commit 3241929b67d2 ("usb: host: xhci: mvebu: make USB 3.0 PHY optional for
Armada 3720")
commit b0c6ae0f8948 ("PCI: aardvark: Fix initialization with old Marvell's
Arm Trusted Firmware")

Replace this RPC implementation with proper native kernel implementation,
which is independent on the firmware. Never return -EOPNOTSUPP for proper
arguments.

This should solve multiple issues with real-world boards, where it is not
possible or really inconvenient to change the firmware. Let's eliminate
these issues.

This implementation is ported directly from Armada 3720 comphy driver found
in newest version of ARM Trusted Firmware source code, but with various
fixes of register names, some added comments, some refactoring due to the
original code not conforming to kernel standards. Also PCIe mode poweroff
support was added here, and PHY reset support. These changes are also going
to be sent to ARM Trusted Firmware.

Signed-off-by: Pali Rohár <pali@kernel.org>
Acked-by: Miquel Raynal <miquel.raynal@bootlin.com>
[ Pali did the porting from ATF.
  I (Marek) then fixed some register names, some various other things,
  added some comments and refactored the code to kernel standards. Also
  fixed PHY poweroff and added PHY reset. ]
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/phy/marvell/phy-mvebu-a3700-comphy.c | 1351 ++++++++++++++++--
 1 file changed, 1234 insertions(+), 117 deletions(-)

--- a/drivers/phy/marvell/phy-mvebu-a3700-comphy.c
+++ b/drivers/phy/marvell/phy-mvebu-a3700-comphy.c
@@ -5,12 +5,16 @@
  * Authors:
  *   Evan Wang <xswang@marvell.com>
  *   Miquèl Raynal <miquel.raynal@bootlin.com>
+ *   Pali Rohár <pali@kernel.org>
+ *   Marek Behún <kabel@kernel.org>
  *
  * Structure inspired from phy-mvebu-cp110-comphy.c written by Antoine Tenart.
- * SMC call initial support done by Grzegorz Jaszczyk.
+ * Comphy code from ARM Trusted Firmware ported by Pali Rohár <pali@kernel.org>
+ * and Marek Behún <kabel@kernel.org>.
  */
 
-#include <linux/arm-smccc.h>
+#include <linux/bitfield.h>
+#include <linux/clk.h>
 #include <linux/io.h>
 #include <linux/iopoll.h>
 #include <linux/mfd/syscon.h>
@@ -18,103 +22,1147 @@
 #include <linux/phy.h>
 #include <linux/phy/phy.h>
 #include <linux/platform_device.h>
+#include <linux/spinlock.h>
 
-#define MVEBU_A3700_COMPHY_LANES		3
+#define PLL_SET_DELAY_US		600
+#define COMPHY_PLL_SLEEP		1000
+#define COMPHY_PLL_TIMEOUT		150000
+
+/* Comphy lane2 indirect access register offset */
+#define COMPHY_LANE2_INDIR_ADDR		0x0
+#define COMPHY_LANE2_INDIR_DATA		0x4
+
+/* SATA and USB3 PHY offset compared to SATA PHY */
+#define COMPHY_LANE2_REGS_BASE		0x200
+
+/*
+ * When accessing common PHY lane registers directly, we need to shift by 1,
+ * since the registers are 16-bit.
+ */
+#define COMPHY_LANE_REG_DIRECT(reg)	(((reg) & 0x7FF) << 1)
+
+/* COMPHY registers */
+#define COMPHY_POWER_PLL_CTRL		0x01
+#define PU_IVREF_BIT			BIT(15)
+#define PU_PLL_BIT			BIT(14)
+#define PU_RX_BIT			BIT(13)
+#define PU_TX_BIT			BIT(12)
+#define PU_TX_INTP_BIT			BIT(11)
+#define PU_DFE_BIT			BIT(10)
+#define RESET_DTL_RX_BIT		BIT(9)
+#define PLL_LOCK_BIT			BIT(8)
+#define REF_FREF_SEL_MASK		GENMASK(4, 0)
+#define REF_FREF_SEL_SERDES_25MHZ	FIELD_PREP(REF_FREF_SEL_MASK, 0x1)
+#define REF_FREF_SEL_SERDES_40MHZ	FIELD_PREP(REF_FREF_SEL_MASK, 0x3)
+#define REF_FREF_SEL_SERDES_50MHZ	FIELD_PREP(REF_FREF_SEL_MASK, 0x4)
+#define REF_FREF_SEL_PCIE_USB3_25MHZ	FIELD_PREP(REF_FREF_SEL_MASK, 0x2)
+#define REF_FREF_SEL_PCIE_USB3_40MHZ	FIELD_PREP(REF_FREF_SEL_MASK, 0x3)
+#define COMPHY_MODE_MASK		GENMASK(7, 5)
+#define COMPHY_MODE_SATA		FIELD_PREP(COMPHY_MODE_MASK, 0x0)
+#define COMPHY_MODE_PCIE		FIELD_PREP(COMPHY_MODE_MASK, 0x3)
+#define COMPHY_MODE_SERDES		FIELD_PREP(COMPHY_MODE_MASK, 0x4)
+#define COMPHY_MODE_USB3		FIELD_PREP(COMPHY_MODE_MASK, 0x5)
+
+#define COMPHY_KVCO_CAL_CTRL		0x02
+#define USE_MAX_PLL_RATE_BIT		BIT(12)
+#define SPEED_PLL_MASK			GENMASK(7, 2)
+#define SPEED_PLL_VALUE_16		FIELD_PREP(SPEED_PLL_MASK, 0x10)
+
+#define COMPHY_DIG_LOOPBACK_EN		0x23
+#define SEL_DATA_WIDTH_MASK		GENMASK(11, 10)
+#define DATA_WIDTH_10BIT		FIELD_PREP(SEL_DATA_WIDTH_MASK, 0x0)
+#define DATA_WIDTH_20BIT		FIELD_PREP(SEL_DATA_WIDTH_MASK, 0x1)
+#define DATA_WIDTH_40BIT		FIELD_PREP(SEL_DATA_WIDTH_MASK, 0x2)
+#define PLL_READY_TX_BIT		BIT(4)
+
+#define COMPHY_SYNC_PATTERN		0x24
+#define TXD_INVERT_BIT			BIT(10)
+#define RXD_INVERT_BIT			BIT(11)
+
+#define COMPHY_SYNC_MASK_GEN		0x25
+#define PHY_GEN_MAX_MASK		GENMASK(11, 10)
+#define PHY_GEN_MAX_USB3_5G		FIELD_PREP(PHY_GEN_MAX_MASK, 0x1)
+
+#define COMPHY_ISOLATION_CTRL		0x26
+#define PHY_ISOLATE_MODE		BIT(15)
+
+#define COMPHY_GEN2_SET2		0x3e
+#define GS2_TX_SSC_AMP_MASK		GENMASK(15, 9)
+#define GS2_TX_SSC_AMP_4128		FIELD_PREP(GS2_TX_SSC_AMP_MASK, 0x20)
+#define GS2_VREG_RXTX_MAS_ISET_MASK	GENMASK(8, 7)
+#define GS2_VREG_RXTX_MAS_ISET_60U	FIELD_PREP(GS2_VREG_RXTX_MAS_ISET_MASK,\
+						   0x0)
+#define GS2_VREG_RXTX_MAS_ISET_80U	FIELD_PREP(GS2_VREG_RXTX_MAS_ISET_MASK,\
+						   0x1)
+#define GS2_VREG_RXTX_MAS_ISET_100U	FIELD_PREP(GS2_VREG_RXTX_MAS_ISET_MASK,\
+						   0x2)
+#define GS2_VREG_RXTX_MAS_ISET_120U	FIELD_PREP(GS2_VREG_RXTX_MAS_ISET_MASK,\
+						   0x3)
+#define GS2_RSVD_6_0_MASK		GENMASK(6, 0)
+
+#define COMPHY_GEN3_SET2		0x3f
+
+#define COMPHY_IDLE_SYNC_EN		0x48
+#define IDLE_SYNC_EN			BIT(12)
+
+#define COMPHY_MISC_CTRL0		0x4F
+#define CLK100M_125M_EN			BIT(4)
+#define TXDCLK_2X_SEL			BIT(6)
+#define CLK500M_EN			BIT(7)
+#define PHY_REF_CLK_SEL			BIT(10)
+
+#define COMPHY_SFT_RESET		0x52
+#define SFT_RST				BIT(9)
+#define SFT_RST_NO_REG			BIT(10)
+
+#define COMPHY_MISC_CTRL1		0x73
+#define SEL_BITS_PCIE_FORCE		BIT(15)
+
+#define COMPHY_GEN2_SET3		0x112
+#define GS3_FFE_CAP_SEL_MASK		GENMASK(3, 0)
+#define GS3_FFE_CAP_SEL_VALUE		FIELD_PREP(GS3_FFE_CAP_SEL_MASK, 0xF)
+
+/* PIPE registers */
+#define COMPHY_PIPE_LANE_CFG0		0x180
+#define PRD_TXDEEMPH0_MASK		BIT(0)
+#define PRD_TXMARGIN_MASK		GENMASK(3, 1)
+#define PRD_TXSWING_MASK		BIT(4)
+#define CFG_TX_ALIGN_POS_MASK		GENMASK(8, 5)
+
+#define COMPHY_PIPE_LANE_CFG1		0x181
+#define PRD_TXDEEMPH1_MASK		BIT(15)
+#define USE_MAX_PLL_RATE_EN		BIT(9)
+#define TX_DET_RX_MODE			BIT(6)
+#define GEN2_TX_DATA_DLY_MASK		GENMASK(4, 3)
+#define GEN2_TX_DATA_DLY_DEFT		FIELD_PREP(GEN2_TX_DATA_DLY_MASK, 2)
+#define TX_ELEC_IDLE_MODE_EN		BIT(0)
+
+#define COMPHY_PIPE_LANE_STAT1		0x183
+#define TXDCLK_PCLK_EN			BIT(0)
+
+#define COMPHY_PIPE_LANE_CFG4		0x188
+#define SPREAD_SPECTRUM_CLK_EN		BIT(7)
+
+#define COMPHY_PIPE_RST_CLK_CTRL	0x1C1
+#define PIPE_SOFT_RESET			BIT(0)
+#define PIPE_REG_RESET			BIT(1)
+#define MODE_CORE_CLK_FREQ_SEL		BIT(9)
+#define MODE_PIPE_WIDTH_32		BIT(3)
+#define MODE_REFDIV_MASK		GENMASK(5, 4)
+#define MODE_REFDIV_BY_4		FIELD_PREP(MODE_REFDIV_MASK, 0x2)
+
+#define COMPHY_PIPE_TEST_MODE_CTRL	0x1C2
+#define MODE_MARGIN_OVERRIDE		BIT(2)
+
+#define COMPHY_PIPE_CLK_SRC_LO		0x1C3
+#define MODE_CLK_SRC			BIT(0)
+#define BUNDLE_PERIOD_SEL		BIT(1)
+#define BUNDLE_PERIOD_SCALE_MASK	GENMASK(3, 2)
+#define BUNDLE_SAMPLE_CTRL		BIT(4)
+#define PLL_READY_DLY_MASK		GENMASK(7, 5)
+#define CFG_SEL_20B			BIT(15)
+
+#define COMPHY_PIPE_PWR_MGM_TIM1	0x1D0
+#define CFG_PM_OSCCLK_WAIT_MASK		GENMASK(15, 12)
+#define CFG_PM_RXDEN_WAIT_MASK		GENMASK(11, 8)
+#define CFG_PM_RXDEN_WAIT_1_UNIT	FIELD_PREP(CFG_PM_RXDEN_WAIT_MASK, 0x1)
+#define CFG_PM_RXDLOZ_WAIT_MASK		GENMASK(7, 0)
+#define CFG_PM_RXDLOZ_WAIT_7_UNIT	FIELD_PREP(CFG_PM_RXDLOZ_WAIT_MASK, 0x7)
+#define CFG_PM_RXDLOZ_WAIT_12_UNIT	FIELD_PREP(CFG_PM_RXDLOZ_WAIT_MASK, 0xC)
+
+/*
+ * This register is not from PHY lane register space. It only exists in the
+ * indirect register space, before the actual PHY lane 2 registers. So the
+ * offset is absolute, not relative to COMPHY_LANE2_REGS_BASE.
+ * It is used only for SATA PHY initialization.
+ */
+#define COMPHY_RESERVED_REG		0x0E
+#define PHYCTRL_FRM_PIN_BIT		BIT(13)
 
-/* COMPHY Fast SMC function identifiers */
-#define COMPHY_SIP_POWER_ON			0x82000001
-#define COMPHY_SIP_POWER_OFF			0x82000002
-#define COMPHY_SIP_PLL_LOCK			0x82000003
-
-#define COMPHY_FW_MODE_SATA			0x1
-#define COMPHY_FW_MODE_SGMII			0x2
-#define COMPHY_FW_MODE_2500BASEX		0x3
-#define COMPHY_FW_MODE_USB3H			0x4
-#define COMPHY_FW_MODE_USB3D			0x5
-#define COMPHY_FW_MODE_PCIE			0x6
-#define COMPHY_FW_MODE_USB3			0xa
-
-#define COMPHY_FW_SPEED_1_25G			0 /* SGMII 1G */
-#define COMPHY_FW_SPEED_2_5G			1
-#define COMPHY_FW_SPEED_3_125G			2 /* 2500BASE-X */
-#define COMPHY_FW_SPEED_5G			3
-#define COMPHY_FW_SPEED_MAX			0x3F
-
-#define COMPHY_FW_MODE(mode)			((mode) << 12)
-#define COMPHY_FW_NET(mode, idx, speed)		(COMPHY_FW_MODE(mode) | \
-						 ((idx) << 8) |	\
-						 ((speed) << 2))
-#define COMPHY_FW_PCIE(mode, speed, width)	(COMPHY_FW_NET(mode, 0, speed) | \
-						 ((width) << 18))
+/* South Bridge PHY Configuration Registers */
+#define COMPHY_PHY_REG(lane, reg)	(((1 - (lane)) * 0x28) + ((reg) & 0x3f))
+
+/*
+ * lane0: USB3/GbE1 PHY Configuration 1
+ * lane1: PCIe/GbE0 PHY Configuration 1
+ * (used only by SGMII code)
+ */
+#define COMPHY_PHY_CFG1			0x0
+#define PIN_PU_IVREF_BIT		BIT(1)
+#define PIN_RESET_CORE_BIT		BIT(11)
+#define PIN_RESET_COMPHY_BIT		BIT(12)
+#define PIN_PU_PLL_BIT			BIT(16)
+#define PIN_PU_RX_BIT			BIT(17)
+#define PIN_PU_TX_BIT			BIT(18)
+#define PIN_TX_IDLE_BIT			BIT(19)
+#define GEN_RX_SEL_MASK			GENMASK(25, 22)
+#define GEN_RX_SEL_VALUE(val)		FIELD_PREP(GEN_RX_SEL_MASK, (val))
+#define GEN_TX_SEL_MASK			GENMASK(29, 26)
+#define GEN_TX_SEL_VALUE(val)		FIELD_PREP(GEN_TX_SEL_MASK, (val))
+#define SERDES_SPEED_1_25_G		0x6
+#define SERDES_SPEED_3_125_G		0x8
+#define PHY_RX_INIT_BIT			BIT(30)
+
+/*
+ * lane0: USB3/GbE1 PHY Status 1
+ * lane1: PCIe/GbE0 PHY Status 1
+ * (used only by SGMII code)
+ */
+#define COMPHY_PHY_STAT1		0x18
+#define PHY_RX_INIT_DONE_BIT		BIT(0)
+#define PHY_PLL_READY_RX_BIT		BIT(2)
+#define PHY_PLL_READY_TX_BIT		BIT(3)
+
+/* PHY Selector */
+#define COMPHY_SELECTOR_PHY_REG			0xFC
+/* bit0: 0: Lane1 is GbE0; 1: Lane1 is PCIe */
+#define COMPHY_SELECTOR_PCIE_GBE0_SEL_BIT	BIT(0)
+/* bit4: 0: Lane0 is GbE1; 1: Lane0 is USB3 */
+#define COMPHY_SELECTOR_USB3_GBE1_SEL_BIT	BIT(4)
+/* bit8: 0: Lane0 is USB3 instead of GbE1, Lane2 is SATA; 1: Lane2 is USB3 */
+#define COMPHY_SELECTOR_USB3_PHY_SEL_BIT	BIT(8)
 
 struct mvebu_a3700_comphy_conf {
 	unsigned int lane;
 	enum phy_mode mode;
 	int submode;
-	u32 fw_mode;
 };
 
-#define MVEBU_A3700_COMPHY_CONF(_lane, _mode, _smode, _fw)		\
+#define MVEBU_A3700_COMPHY_CONF(_lane, _mode, _smode)			\
 	{								\
 		.lane = _lane,						\
 		.mode = _mode,						\
 		.submode = _smode,					\
-		.fw_mode = _fw,						\
 	}
 
-#define MVEBU_A3700_COMPHY_CONF_GEN(_lane, _mode, _fw) \
-	MVEBU_A3700_COMPHY_CONF(_lane, _mode, PHY_INTERFACE_MODE_NA, _fw)
+#define MVEBU_A3700_COMPHY_CONF_GEN(_lane, _mode) \
+	MVEBU_A3700_COMPHY_CONF(_lane, _mode, PHY_INTERFACE_MODE_NA)
 
-#define MVEBU_A3700_COMPHY_CONF_ETH(_lane, _smode, _fw) \
-	MVEBU_A3700_COMPHY_CONF(_lane, PHY_MODE_ETHERNET, _smode, _fw)
+#define MVEBU_A3700_COMPHY_CONF_ETH(_lane, _smode) \
+	MVEBU_A3700_COMPHY_CONF(_lane, PHY_MODE_ETHERNET, _smode)
 
 static const struct mvebu_a3700_comphy_conf mvebu_a3700_comphy_modes[] = {
 	/* lane 0 */
-	MVEBU_A3700_COMPHY_CONF_GEN(0, PHY_MODE_USB_HOST_SS,
-				    COMPHY_FW_MODE_USB3H),
-	MVEBU_A3700_COMPHY_CONF_ETH(0, PHY_INTERFACE_MODE_SGMII,
-				    COMPHY_FW_MODE_SGMII),
-	MVEBU_A3700_COMPHY_CONF_ETH(0, PHY_INTERFACE_MODE_2500BASEX,
-				    COMPHY_FW_MODE_2500BASEX),
+	MVEBU_A3700_COMPHY_CONF_GEN(0, PHY_MODE_USB_HOST_SS),
+	MVEBU_A3700_COMPHY_CONF_ETH(0, PHY_INTERFACE_MODE_SGMII),
+	MVEBU_A3700_COMPHY_CONF_ETH(0, PHY_INTERFACE_MODE_1000BASEX),
+	MVEBU_A3700_COMPHY_CONF_ETH(0, PHY_INTERFACE_MODE_2500BASEX),
 	/* lane 1 */
-	MVEBU_A3700_COMPHY_CONF_GEN(1, PHY_MODE_PCIE, COMPHY_FW_MODE_PCIE),
-	MVEBU_A3700_COMPHY_CONF_ETH(1, PHY_INTERFACE_MODE_SGMII,
-				    COMPHY_FW_MODE_SGMII),
-	MVEBU_A3700_COMPHY_CONF_ETH(1, PHY_INTERFACE_MODE_2500BASEX,
-				    COMPHY_FW_MODE_2500BASEX),
+	MVEBU_A3700_COMPHY_CONF_GEN(1, PHY_MODE_PCIE),
+	MVEBU_A3700_COMPHY_CONF_ETH(1, PHY_INTERFACE_MODE_SGMII),
+	MVEBU_A3700_COMPHY_CONF_ETH(1, PHY_INTERFACE_MODE_1000BASEX),
+	MVEBU_A3700_COMPHY_CONF_ETH(1, PHY_INTERFACE_MODE_2500BASEX),
 	/* lane 2 */
-	MVEBU_A3700_COMPHY_CONF_GEN(2, PHY_MODE_SATA, COMPHY_FW_MODE_SATA),
-	MVEBU_A3700_COMPHY_CONF_GEN(2, PHY_MODE_USB_HOST_SS,
-				    COMPHY_FW_MODE_USB3H),
+	MVEBU_A3700_COMPHY_CONF_GEN(2, PHY_MODE_SATA),
+	MVEBU_A3700_COMPHY_CONF_GEN(2, PHY_MODE_USB_HOST_SS),
+};
+
+struct mvebu_a3700_comphy_priv {
+	void __iomem *comphy_regs;
+	void __iomem *lane0_phy_regs; /* USB3 and GbE1 */
+	void __iomem *lane1_phy_regs; /* PCIe and GbE0 */
+	void __iomem *lane2_phy_indirect; /* SATA and USB3 */
+	spinlock_t lock; /* for PHY selector access */
+	bool xtal_is_40m;
 };
 
 struct mvebu_a3700_comphy_lane {
+	struct mvebu_a3700_comphy_priv *priv;
 	struct device *dev;
 	unsigned int id;
 	enum phy_mode mode;
 	int submode;
+	bool invert_tx;
+	bool invert_rx;
+	bool needs_reset;
+};
+
+struct gbe_phy_init_data_fix {
+	u16 addr;
+	u16 value;
+};
+
+/* Changes to 40M1G25 mode data required for running 40M3G125 init mode */
+static struct gbe_phy_init_data_fix gbe_phy_init_fix[] = {
+	{ 0x005, 0x07CC }, { 0x015, 0x0000 }, { 0x01B, 0x0000 },
+	{ 0x01D, 0x0000 }, { 0x01E, 0x0000 }, { 0x01F, 0x0000 },
+	{ 0x020, 0x0000 }, { 0x021, 0x0030 }, { 0x026, 0x0888 },
+	{ 0x04D, 0x0152 }, { 0x04F, 0xA020 }, { 0x050, 0x07CC },
+	{ 0x053, 0xE9CA }, { 0x055, 0xBD97 }, { 0x071, 0x3015 },
+	{ 0x076, 0x03AA }, { 0x07C, 0x0FDF }, { 0x0C2, 0x3030 },
+	{ 0x0C3, 0x8000 }, { 0x0E2, 0x5550 }, { 0x0E3, 0x12A4 },
+	{ 0x0E4, 0x7D00 }, { 0x0E6, 0x0C83 }, { 0x101, 0xFCC0 },
+	{ 0x104, 0x0C10 }
 };
 
-static int mvebu_a3700_comphy_smc(unsigned long function, unsigned long lane,
-				  unsigned long mode)
+/* 40M1G25 mode init data */
+static u16 gbe_phy_init[512] = {
+	/* 0       1       2       3       4       5       6       7 */
+	/*-----------------------------------------------------------*/
+	/* 8       9       A       B       C       D       E       F */
+	0x3110, 0xFD83, 0x6430, 0x412F, 0x82C0, 0x06FA, 0x4500, 0x6D26,	/* 00 */
+	0xAFC0, 0x8000, 0xC000, 0x0000, 0x2000, 0x49CC, 0x0BC9, 0x2A52,	/* 08 */
+	0x0BD2, 0x0CDE, 0x13D2, 0x0CE8, 0x1149, 0x10E0, 0x0000, 0x0000,	/* 10 */
+	0x0000, 0x0000, 0x0000, 0x0001, 0x0000, 0x4134, 0x0D2D, 0xFFFF,	/* 18 */
+	0xFFE0, 0x4030, 0x1016, 0x0030, 0x0000, 0x0800, 0x0866, 0x0000,	/* 20 */
+	0x0000, 0x0000, 0xFFFF, 0xFFFF, 0xFFFF, 0xFFFF, 0xFFFF, 0xFFFF,	/* 28 */
+	0xFFFF, 0xFFFF, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/* 30 */
+	0x0000, 0x0000, 0x000F, 0x6A62, 0x1988, 0x3100, 0x3100, 0x3100,	/* 38 */
+	0x3100, 0xA708, 0x2430, 0x0830, 0x1030, 0x4610, 0xFF00, 0xFF00,	/* 40 */
+	0x0060, 0x1000, 0x0400, 0x0040, 0x00F0, 0x0155, 0x1100, 0xA02A,	/* 48 */
+	0x06FA, 0x0080, 0xB008, 0xE3ED, 0x5002, 0xB592, 0x7A80, 0x0001,	/* 50 */
+	0x020A, 0x8820, 0x6014, 0x8054, 0xACAA, 0xFC88, 0x2A02, 0x45CF,	/* 58 */
+	0x000F, 0x1817, 0x2860, 0x064F, 0x0000, 0x0204, 0x1800, 0x6000,	/* 60 */
+	0x810F, 0x4F23, 0x4000, 0x4498, 0x0850, 0x0000, 0x000E, 0x1002,	/* 68 */
+	0x9D3A, 0x3009, 0xD066, 0x0491, 0x0001, 0x6AB0, 0x0399, 0x3780,	/* 70 */
+	0x0040, 0x5AC0, 0x4A80, 0x0000, 0x01DF, 0x0000, 0x0007, 0x0000,	/* 78 */
+	0x2D54, 0x00A1, 0x4000, 0x0100, 0xA20A, 0x0000, 0x0000, 0x0000,	/* 80 */
+	0x0000, 0x0000, 0x0000, 0x7400, 0x0E81, 0x1000, 0x1242, 0x0210,	/* 88 */
+	0x80DF, 0x0F1F, 0x2F3F, 0x4F5F, 0x6F7F, 0x0F1F, 0x2F3F, 0x4F5F,	/* 90 */
+	0x6F7F, 0x4BAD, 0x0000, 0x0000, 0x0800, 0x0000, 0x2400, 0xB651,	/* 98 */
+	0xC9E0, 0x4247, 0x0A24, 0x0000, 0xAF19, 0x1004, 0x0000, 0x0000,	/* A0 */
+	0x0000, 0x0013, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/* A8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/* B0 */
+	0x0000, 0x0000, 0x0000, 0x0060, 0x0000, 0x0000, 0x0000, 0x0000,	/* B8 */
+	0x0000, 0x0000, 0x3010, 0xFA00, 0x0000, 0x0000, 0x0000, 0x0003,	/* C0 */
+	0x1618, 0x8200, 0x8000, 0x0400, 0x050F, 0x0000, 0x0000, 0x0000,	/* C8 */
+	0x4C93, 0x0000, 0x1000, 0x1120, 0x0010, 0x1242, 0x1242, 0x1E00,	/* D0 */
+	0x0000, 0x0000, 0x0000, 0x00F8, 0x0000, 0x0041, 0x0800, 0x0000,	/* D8 */
+	0x82A0, 0x572E, 0x2490, 0x14A9, 0x4E00, 0x0000, 0x0803, 0x0541,	/* E0 */
+	0x0C15, 0x0000, 0x0000, 0x0400, 0x2626, 0x0000, 0x0000, 0x4200,	/* E8 */
+	0x0000, 0xAA55, 0x1020, 0x0000, 0x0000, 0x5010, 0x0000, 0x0000,	/* F0 */
+	0x0000, 0x0000, 0x5000, 0x0000, 0x0000, 0x0000, 0x02F2, 0x0000,	/* F8 */
+	0x101F, 0xFDC0, 0x4000, 0x8010, 0x0110, 0x0006, 0x0000, 0x0000,	/*100 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*108 */
+	0x04CF, 0x0000, 0x04CF, 0x0000, 0x04CF, 0x0000, 0x04C6, 0x0000,	/*110 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*118 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*120 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*128 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*130 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*138 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*140 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*148 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*150 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*158 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*160 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*168 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*170 */
+	0x0000, 0x0000, 0x0000, 0x00F0, 0x08A2, 0x3112, 0x0A14, 0x0000,	/*178 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*180 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*188 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*190 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*198 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1A0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1A8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1B0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1B8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1C0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1C8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1D0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1D8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1E0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1E8 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000,	/*1F0 */
+	0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000	/*1F8 */
+};
+
+static inline void comphy_reg_set(void __iomem *addr, u32 data, u32 mask)
 {
-	struct arm_smccc_res res;
-	s32 ret;
+	u32 val;
 
-	arm_smccc_smc(function, lane, mode, 0, 0, 0, 0, 0, &res);
-	ret = res.a0;
+	val = readl(addr);
+	val = (val & ~mask) | (data & mask);
+	writel(val, addr);
+}
 
-	switch (ret) {
-	case SMCCC_RET_SUCCESS:
-		return 0;
-	case SMCCC_RET_NOT_SUPPORTED:
-		return -EOPNOTSUPP;
+static inline void comphy_reg_set16(void __iomem *addr, u16 data, u16 mask)
+{
+	u16 val;
+
+	val = readw(addr);
+	val = (val & ~mask) | (data & mask);
+	writew(val, addr);
+}
+
+/* Used for accessing lane 2 registers (SATA/USB3 PHY) */
+static void comphy_set_indirect(struct mvebu_a3700_comphy_priv *priv,
+				u32 offset, u16 data, u16 mask)
+{
+	writel(offset,
+	       priv->lane2_phy_indirect + COMPHY_LANE2_INDIR_ADDR);
+	comphy_reg_set(priv->lane2_phy_indirect + COMPHY_LANE2_INDIR_DATA,
+		       data, mask);
+}
+
+static void comphy_lane_reg_set(struct mvebu_a3700_comphy_lane *lane,
+				u16 reg, u16 data, u16 mask)
+{
+	if (lane->id == 2) {
+		/* lane 2 PHY registers are accessed indirectly */
+		comphy_set_indirect(lane->priv,
+				    reg + COMPHY_LANE2_REGS_BASE,
+				    data, mask);
+	} else {
+		void __iomem *base = lane->id == 1 ?
+				     lane->priv->lane1_phy_regs :
+				     lane->priv->lane0_phy_regs;
+
+		comphy_reg_set16(base + COMPHY_LANE_REG_DIRECT(reg),
+				 data, mask);
+	}
+}
+
+static int comphy_lane_reg_poll(struct mvebu_a3700_comphy_lane *lane,
+				u16 reg, u16 bits,
+				ulong sleep_us, ulong timeout_us)
+{
+	int ret;
+
+	if (lane->id == 2) {
+		u32 data;
+
+		/* lane 2 PHY registers are accessed indirectly */
+		writel(reg + COMPHY_LANE2_REGS_BASE,
+		       lane->priv->lane2_phy_indirect +
+		       COMPHY_LANE2_INDIR_ADDR);
+
+		ret = readl_poll_timeout(lane->priv->lane2_phy_indirect +
+					 COMPHY_LANE2_INDIR_DATA,
+					 data, (data & bits) == bits,
+					 sleep_us, timeout_us);
+	} else {
+		void __iomem *base = lane->id == 1 ?
+				     lane->priv->lane1_phy_regs :
+				     lane->priv->lane0_phy_regs;
+		u16 data;
+
+		ret = readw_poll_timeout(base + COMPHY_LANE_REG_DIRECT(reg),
+					 data, (data & bits) == bits,
+					 sleep_us, timeout_us);
+	}
+
+	return ret;
+}
+
+static void comphy_periph_reg_set(struct mvebu_a3700_comphy_lane *lane,
+				  u8 reg, u32 data, u32 mask)
+{
+	comphy_reg_set(lane->priv->comphy_regs + COMPHY_PHY_REG(lane->id, reg),
+		       data, mask);
+}
+
+static int comphy_periph_reg_poll(struct mvebu_a3700_comphy_lane *lane,
+				  u8 reg, u32 bits,
+				  ulong sleep_us, ulong timeout_us)
+{
+	u32 data;
+
+	return readl_poll_timeout(lane->priv->comphy_regs +
+				  COMPHY_PHY_REG(lane->id, reg),
+				  data, (data & bits) == bits,
+				  sleep_us, timeout_us);
+}
+
+/* PHY selector configures with corresponding modes */
+static int
+mvebu_a3700_comphy_set_phy_selector(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 old, new, clr = 0, set = 0;
+	unsigned long flags;
+
+	switch (lane->mode) {
+	case PHY_MODE_SATA:
+		/* SATA must be in Lane2 */
+		if (lane->id == 2)
+			clr = COMPHY_SELECTOR_USB3_PHY_SEL_BIT;
+		else
+			goto error;
+		break;
+
+	case PHY_MODE_ETHERNET:
+		if (lane->id == 0)
+			clr = COMPHY_SELECTOR_USB3_GBE1_SEL_BIT;
+		else if (lane->id == 1)
+			clr = COMPHY_SELECTOR_PCIE_GBE0_SEL_BIT;
+		else
+			goto error;
+		break;
+
+	case PHY_MODE_USB_HOST_SS:
+		if (lane->id == 2)
+			set = COMPHY_SELECTOR_USB3_PHY_SEL_BIT;
+		else if (lane->id == 0)
+			set = COMPHY_SELECTOR_USB3_GBE1_SEL_BIT;
+		else
+			goto error;
+		break;
+
+	case PHY_MODE_PCIE:
+		/* PCIE must be in Lane1 */
+		if (lane->id == 1)
+			set = COMPHY_SELECTOR_PCIE_GBE0_SEL_BIT;
+		else
+			goto error;
+		break;
+
+	default:
+		goto error;
+	}
+
+	spin_lock_irqsave(&lane->priv->lock, flags);
+
+	old = readl(lane->priv->comphy_regs + COMPHY_SELECTOR_PHY_REG);
+	new = (old & ~clr) | set;
+	writel(new, lane->priv->comphy_regs + COMPHY_SELECTOR_PHY_REG);
+
+	spin_unlock_irqrestore(&lane->priv->lock, flags);
+
+	dev_dbg(lane->dev,
+		"COMPHY[%d] mode[%d] changed PHY selector 0x%08x -> 0x%08x\n",
+		lane->id, lane->mode, old, new);
+
+	return 0;
+error:
+	dev_err(lane->dev, "COMPHY[%d] mode[%d] is invalid\n", lane->id,
+		lane->mode);
+	return -EINVAL;
+}
+
+static int
+mvebu_a3700_comphy_sata_power_on(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 mask, data, ref_clk;
+	int ret;
+
+	/* Configure phy selector for SATA */
+	ret = mvebu_a3700_comphy_set_phy_selector(lane);
+	if (ret)
+		return ret;
+
+	/* Clear phy isolation mode to make it work in normal mode */
+	comphy_lane_reg_set(lane, COMPHY_ISOLATION_CTRL,
+			    0x0, PHY_ISOLATE_MODE);
+
+	/* 0. Check the Polarity invert bits */
+	data = 0x0;
+	if (lane->invert_tx)
+		data |= TXD_INVERT_BIT;
+	if (lane->invert_rx)
+		data |= RXD_INVERT_BIT;
+	mask = TXD_INVERT_BIT | RXD_INVERT_BIT;
+	comphy_lane_reg_set(lane, COMPHY_SYNC_PATTERN, data, mask);
+
+	/* 1. Select 40-bit data width */
+	comphy_lane_reg_set(lane, COMPHY_DIG_LOOPBACK_EN,
+			    DATA_WIDTH_40BIT, SEL_DATA_WIDTH_MASK);
+
+	/* 2. Select reference clock(25M) and PHY mode (SATA) */
+	if (lane->priv->xtal_is_40m)
+		ref_clk = REF_FREF_SEL_SERDES_40MHZ;
+	else
+		ref_clk = REF_FREF_SEL_SERDES_25MHZ;
+
+	data = ref_clk | COMPHY_MODE_SATA;
+	mask = REF_FREF_SEL_MASK | COMPHY_MODE_MASK;
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL, data, mask);
+
+	/* 3. Use maximum PLL rate (no power save) */
+	comphy_lane_reg_set(lane, COMPHY_KVCO_CAL_CTRL,
+			    USE_MAX_PLL_RATE_BIT, USE_MAX_PLL_RATE_BIT);
+
+	/* 4. Reset reserved bit */
+	comphy_set_indirect(lane->priv, COMPHY_RESERVED_REG,
+			    0x0, PHYCTRL_FRM_PIN_BIT);
+
+	/* 5. Set vendor-specific configuration (It is done in sata driver) */
+	/* XXX: in U-Boot below sequence was executed in this place, in Linux
+	 * not.  Now it is done only in U-Boot before this comphy
+	 * initialization - tests shows that it works ok, but in case of any
+	 * future problem it is left for reference.
+	 *   reg_set(MVEBU_REGS_BASE + 0xe00a0, 0, 0xffffffff);
+	 *   reg_set(MVEBU_REGS_BASE + 0xe00a4, BIT(6), BIT(6));
+	 */
+
+	/* Wait for > 55 us to allow PLL be enabled */
+	udelay(PLL_SET_DELAY_US);
+
+	/* Polling status */
+	ret = comphy_lane_reg_poll(lane, COMPHY_DIG_LOOPBACK_EN,
+				   PLL_READY_TX_BIT, COMPHY_PLL_SLEEP,
+				   COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to lock SATA PLL\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static void comphy_gbe_phy_init(struct mvebu_a3700_comphy_lane *lane,
+				bool is_1gbps)
+{
+	int addr, fix_idx;
+	u16 val;
+
+	fix_idx = 0;
+	for (addr = 0; addr < 512; addr++) {
+		/*
+		 * All PHY register values are defined in full for 3.125Gbps
+		 * SERDES speed. The values required for 1.25 Gbps are almost
+		 * the same and only few registers should be "fixed" in
+		 * comparison to 3.125 Gbps values. These register values are
+		 * stored in "gbe_phy_init_fix" array.
+		 */
+		if (!is_1gbps && gbe_phy_init_fix[fix_idx].addr == addr) {
+			/* Use new value */
+			val = gbe_phy_init_fix[fix_idx].value;
+			if (fix_idx < ARRAY_SIZE(gbe_phy_init_fix))
+				fix_idx++;
+		} else {
+			val = gbe_phy_init[addr];
+		}
+
+		comphy_lane_reg_set(lane, addr, val, 0xFFFF);
+	}
+}
+
+static int
+mvebu_a3700_comphy_ethernet_power_on(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 mask, data, speed_sel;
+	int ret;
+
+	/* Set selector */
+	ret = mvebu_a3700_comphy_set_phy_selector(lane);
+	if (ret)
+		return ret;
+
+	/*
+	 * 1. Reset PHY by setting PHY input port PIN_RESET=1.
+	 * 2. Set PHY input port PIN_TX_IDLE=1, PIN_PU_IVREF=1 to keep
+	 *    PHY TXP/TXN output to idle state during PHY initialization
+	 * 3. Set PHY input port PIN_PU_PLL=0, PIN_PU_RX=0, PIN_PU_TX=0.
+	 */
+	data = PIN_PU_IVREF_BIT | PIN_TX_IDLE_BIT | PIN_RESET_COMPHY_BIT;
+	mask = data | PIN_RESET_CORE_BIT | PIN_PU_PLL_BIT | PIN_PU_RX_BIT |
+	       PIN_PU_TX_BIT | PHY_RX_INIT_BIT;
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+
+	/* 4. Release reset to the PHY by setting PIN_RESET=0. */
+	data = 0x0;
+	mask = PIN_RESET_COMPHY_BIT;
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+
+	/*
+	 * 5. Set PIN_PHY_GEN_TX[3:0] and PIN_PHY_GEN_RX[3:0] to decide COMPHY
+	 * bit rate
+	 */
+	switch (lane->submode) {
+	case PHY_INTERFACE_MODE_SGMII:
+	case PHY_INTERFACE_MODE_1000BASEX:
+		/* SGMII 1G, SerDes speed 1.25G */
+		speed_sel = SERDES_SPEED_1_25_G;
+		break;
+	case PHY_INTERFACE_MODE_2500BASEX:
+		/* 2500Base-X, SerDes speed 3.125G */
+		speed_sel = SERDES_SPEED_3_125_G;
+		break;
 	default:
+		/* Other rates are not supported */
+		dev_err(lane->dev,
+			"unsupported phy speed %d on comphy lane%d\n",
+			lane->submode, lane->id);
 		return -EINVAL;
 	}
+	data = GEN_RX_SEL_VALUE(speed_sel) | GEN_TX_SEL_VALUE(speed_sel);
+	mask = GEN_RX_SEL_MASK | GEN_TX_SEL_MASK;
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+
+	/*
+	 * 6. Wait 10mS for bandgap and reference clocks to stabilize; then
+	 * start SW programming.
+	 */
+	mdelay(10);
+
+	/* 7. Program COMPHY register PHY_MODE */
+	data = COMPHY_MODE_SERDES;
+	mask = COMPHY_MODE_MASK;
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL, data, mask);
+
+	/*
+	 * 8. Set COMPHY register REFCLK_SEL to select the correct REFCLK
+	 * source
+	 */
+	data = 0x0;
+	mask = PHY_REF_CLK_SEL;
+	comphy_lane_reg_set(lane, COMPHY_MISC_CTRL0, data, mask);
+
+	/*
+	 * 9. Set correct reference clock frequency in COMPHY register
+	 * REF_FREF_SEL.
+	 */
+	if (lane->priv->xtal_is_40m)
+		data = REF_FREF_SEL_SERDES_50MHZ;
+	else
+		data = REF_FREF_SEL_SERDES_25MHZ;
+
+	mask = REF_FREF_SEL_MASK;
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL, data, mask);
+
+	/* 10. Program COMPHY register PHY_GEN_MAX[1:0]
+	 * This step is mentioned in the flow received from verification team.
+	 * However the PHY_GEN_MAX value is only meaningful for other interfaces
+	 * (not SERDES). For instance, it selects SATA speed 1.5/3/6 Gbps or
+	 * PCIe speed 2.5/5 Gbps
+	 */
+
+	/*
+	 * 11. Program COMPHY register SEL_BITS to set correct parallel data
+	 * bus width
+	 */
+	data = DATA_WIDTH_10BIT;
+	mask = SEL_DATA_WIDTH_MASK;
+	comphy_lane_reg_set(lane, COMPHY_DIG_LOOPBACK_EN, data, mask);
+
+	/*
+	 * 12. As long as DFE function needs to be enabled in any mode,
+	 * COMPHY register DFE_UPDATE_EN[5:0] shall be programmed to 0x3F
+	 * for real chip during COMPHY power on.
+	 * The step 14 exists (and empty) in the original initialization flow
+	 * obtained from the verification team. According to the functional
+	 * specification DFE_UPDATE_EN already has the default value 0x3F
+	 */
+
+	/*
+	 * 13. Program COMPHY GEN registers.
+	 * These registers should be programmed based on the lab testing result
+	 * to achieve optimal performance. Please contact the CEA group to get
+	 * the related GEN table during real chip bring-up. We only required to
+	 * run though the entire registers programming flow defined by
+	 * "comphy_gbe_phy_init" when the REF clock is 40 MHz. For REF clock
+	 * 25 MHz the default values stored in PHY registers are OK.
+	 */
+	dev_dbg(lane->dev, "Running C-DPI phy init %s mode\n",
+		lane->submode == PHY_INTERFACE_MODE_2500BASEX ? "2G5" : "1G");
+	if (lane->priv->xtal_is_40m)
+		comphy_gbe_phy_init(lane,
+				    lane->submode != PHY_INTERFACE_MODE_2500BASEX);
+
+	/*
+	 * 14. [Simulation Only] should not be used for real chip.
+	 * By pass power up calibration by programming EXT_FORCE_CAL_DONE
+	 * (R02h[9]) to 1 to shorten COMPHY simulation time.
+	 */
+
+	/*
+	 * 15. [Simulation Only: should not be used for real chip]
+	 * Program COMPHY register FAST_DFE_TIMER_EN=1 to shorten RX training
+	 * simulation time.
+	 */
+
+	/*
+	 * 16. Check the PHY Polarity invert bit
+	 */
+	data = 0x0;
+	if (lane->invert_tx)
+		data |= TXD_INVERT_BIT;
+	if (lane->invert_rx)
+		data |= RXD_INVERT_BIT;
+	mask = TXD_INVERT_BIT | RXD_INVERT_BIT;
+	comphy_lane_reg_set(lane, COMPHY_SYNC_PATTERN, data, mask);
+
+	/*
+	 * 17. Set PHY input ports PIN_PU_PLL, PIN_PU_TX and PIN_PU_RX to 1 to
+	 * start PHY power up sequence. All the PHY register programming should
+	 * be done before PIN_PU_PLL=1. There should be no register programming
+	 * for normal PHY operation from this point.
+	 */
+	data = PIN_PU_PLL_BIT | PIN_PU_RX_BIT | PIN_PU_TX_BIT;
+	mask = data;
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+
+	/*
+	 * 18. Wait for PHY power up sequence to finish by checking output ports
+	 * PIN_PLL_READY_TX=1 and PIN_PLL_READY_RX=1.
+	 */
+	ret = comphy_periph_reg_poll(lane, COMPHY_PHY_STAT1,
+				     PHY_PLL_READY_TX_BIT |
+				     PHY_PLL_READY_RX_BIT,
+				     COMPHY_PLL_SLEEP, COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to lock PLL for SERDES PHY %d\n",
+			lane->id);
+		return ret;
+	}
+
+	/*
+	 * 19. Set COMPHY input port PIN_TX_IDLE=0
+	 */
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, 0x0, PIN_TX_IDLE_BIT);
+
+	/*
+	 * 20. After valid data appear on PIN_RXDATA bus, set PIN_RX_INIT=1. To
+	 * start RX initialization. PIN_RX_INIT_DONE will be cleared to 0 by the
+	 * PHY After RX initialization is done, PIN_RX_INIT_DONE will be set to
+	 * 1 by COMPHY Set PIN_RX_INIT=0 after PIN_RX_INIT_DONE= 1. Please
+	 * refer to RX initialization part for details.
+	 */
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1,
+			      PHY_RX_INIT_BIT, PHY_RX_INIT_BIT);
+
+	ret = comphy_periph_reg_poll(lane, COMPHY_PHY_STAT1,
+				     PHY_PLL_READY_TX_BIT |
+				     PHY_PLL_READY_RX_BIT,
+				     COMPHY_PLL_SLEEP, COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to lock PLL for SERDES PHY %d\n",
+			lane->id);
+		return ret;
+	}
+
+	ret = comphy_periph_reg_poll(lane, COMPHY_PHY_STAT1,
+				     PHY_RX_INIT_DONE_BIT,
+				     COMPHY_PLL_SLEEP, COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to init RX of SERDES PHY %d\n",
+			lane->id);
+		return ret;
+	}
+
+	return 0;
 }
 
-static int mvebu_a3700_comphy_get_fw_mode(int lane,
+static int
+mvebu_a3700_comphy_usb3_power_on(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 mask, data, cfg, ref_clk;
+	int ret;
+
+	/* Set phy seclector */
+	ret = mvebu_a3700_comphy_set_phy_selector(lane);
+	if (ret)
+		return ret;
+
+	/*
+	 * 0. Set PHY OTG Control(0x5d034), bit 4, Power up OTG module The
+	 * register belong to UTMI module, so it is set in UTMI phy driver.
+	 */
+
+	/*
+	 * 1. Set PRD_TXDEEMPH (3.5db de-emph)
+	 */
+	data = PRD_TXDEEMPH0_MASK;
+	mask = PRD_TXDEEMPH0_MASK | PRD_TXMARGIN_MASK | PRD_TXSWING_MASK |
+	       CFG_TX_ALIGN_POS_MASK;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_LANE_CFG0, data, mask);
+
+	/*
+	 * 2. Set BIT0: enable transmitter in high impedance mode
+	 *    Set BIT[3:4]: delay 2 clock cycles for HiZ off latency
+	 *    Set BIT6: Tx detect Rx at HiZ mode
+	 *    Unset BIT15: set to 0 to set USB3 De-emphasize level to -3.5db
+	 *            together with bit 0 of COMPHY_PIPE_LANE_CFG0 register
+	 */
+	data = TX_DET_RX_MODE | GEN2_TX_DATA_DLY_DEFT | TX_ELEC_IDLE_MODE_EN;
+	mask = PRD_TXDEEMPH1_MASK | TX_DET_RX_MODE | GEN2_TX_DATA_DLY_MASK |
+	       TX_ELEC_IDLE_MODE_EN;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_LANE_CFG1, data, mask);
+
+	/*
+	 * 3. Set Spread Spectrum Clock Enabled
+	 */
+	comphy_lane_reg_set(lane, COMPHY_PIPE_LANE_CFG4,
+			    SPREAD_SPECTRUM_CLK_EN, SPREAD_SPECTRUM_CLK_EN);
+
+	/*
+	 * 4. Set Override Margining Controls From the MAC:
+	 *    Use margining signals from lane configuration
+	 */
+	comphy_lane_reg_set(lane, COMPHY_PIPE_TEST_MODE_CTRL,
+			    MODE_MARGIN_OVERRIDE, 0xFFFF);
+
+	/*
+	 * 5. Set Lane-to-Lane Bundle Clock Sampling Period = per PCLK cycles
+	 *    set Mode Clock Source = PCLK is generated from REFCLK
+	 */
+	data = 0x0;
+	mask = MODE_CLK_SRC | BUNDLE_PERIOD_SEL | BUNDLE_PERIOD_SCALE_MASK |
+	       BUNDLE_SAMPLE_CTRL | PLL_READY_DLY_MASK;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_CLK_SRC_LO, data, mask);
+
+	/*
+	 * 6. Set G2 Spread Spectrum Clock Amplitude at 4K
+	 */
+	comphy_lane_reg_set(lane, COMPHY_GEN2_SET2,
+			    GS2_TX_SSC_AMP_4128, GS2_TX_SSC_AMP_MASK);
+
+	/*
+	 * 7. Unset G3 Spread Spectrum Clock Amplitude
+	 *    set G3 TX and RX Register Master Current Select
+	 */
+	data = GS2_VREG_RXTX_MAS_ISET_60U;
+	mask = GS2_TX_SSC_AMP_MASK | GS2_VREG_RXTX_MAS_ISET_MASK |
+	       GS2_RSVD_6_0_MASK;
+	comphy_lane_reg_set(lane, COMPHY_GEN3_SET2, data, mask);
+
+	/*
+	 * 8. Check crystal jumper setting and program the Power and PLL Control
+	 * accordingly Change RX wait
+	 */
+	if (lane->priv->xtal_is_40m) {
+		ref_clk = REF_FREF_SEL_PCIE_USB3_40MHZ;
+		cfg = CFG_PM_RXDLOZ_WAIT_12_UNIT;
+	} else {
+		ref_clk = REF_FREF_SEL_PCIE_USB3_25MHZ;
+		cfg = CFG_PM_RXDLOZ_WAIT_7_UNIT;
+	}
+
+	data = PU_IVREF_BIT | PU_PLL_BIT | PU_RX_BIT | PU_TX_BIT |
+	       PU_TX_INTP_BIT | PU_DFE_BIT | COMPHY_MODE_USB3 | ref_clk;
+	mask = PU_IVREF_BIT | PU_PLL_BIT | PU_RX_BIT | PU_TX_BIT |
+	       PU_TX_INTP_BIT | PU_DFE_BIT | PLL_LOCK_BIT | COMPHY_MODE_MASK |
+	       REF_FREF_SEL_MASK;
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL, data, mask);
+
+	data = CFG_PM_RXDEN_WAIT_1_UNIT | cfg;
+	mask = CFG_PM_OSCCLK_WAIT_MASK | CFG_PM_RXDEN_WAIT_MASK |
+	       CFG_PM_RXDLOZ_WAIT_MASK;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_PWR_MGM_TIM1, data, mask);
+
+	/*
+	 * 9. Enable idle sync
+	 */
+	comphy_lane_reg_set(lane, COMPHY_IDLE_SYNC_EN,
+			    IDLE_SYNC_EN, IDLE_SYNC_EN);
+
+	/*
+	 * 10. Enable the output of 500M clock
+	 */
+	comphy_lane_reg_set(lane, COMPHY_MISC_CTRL0, CLK500M_EN, CLK500M_EN);
+
+	/*
+	 * 11. Set 20-bit data width
+	 */
+	comphy_lane_reg_set(lane, COMPHY_DIG_LOOPBACK_EN,
+			    DATA_WIDTH_20BIT, 0xFFFF);
+
+	/*
+	 * 12. Override Speed_PLL value and use MAC PLL
+	 */
+	data = SPEED_PLL_VALUE_16 | USE_MAX_PLL_RATE_BIT;
+	mask = 0xFFFF;
+	comphy_lane_reg_set(lane, COMPHY_KVCO_CAL_CTRL, data, mask);
+
+	/*
+	 * 13. Check the Polarity invert bit
+	 */
+	data = 0x0;
+	if (lane->invert_tx)
+		data |= TXD_INVERT_BIT;
+	if (lane->invert_rx)
+		data |= RXD_INVERT_BIT;
+	mask = TXD_INVERT_BIT | RXD_INVERT_BIT;
+	comphy_lane_reg_set(lane, COMPHY_SYNC_PATTERN, data, mask);
+
+	/*
+	 * 14. Set max speed generation to USB3.0 5Gbps
+	 */
+	comphy_lane_reg_set(lane, COMPHY_SYNC_MASK_GEN,
+			    PHY_GEN_MAX_USB3_5G, PHY_GEN_MAX_MASK);
+
+	/*
+	 * 15. Set capacitor value for FFE gain peaking to 0xF
+	 */
+	comphy_lane_reg_set(lane, COMPHY_GEN2_SET3,
+			    GS3_FFE_CAP_SEL_VALUE, GS3_FFE_CAP_SEL_MASK);
+
+	/*
+	 * 16. Release SW reset
+	 */
+	data = MODE_CORE_CLK_FREQ_SEL | MODE_PIPE_WIDTH_32 | MODE_REFDIV_BY_4;
+	mask = 0xFFFF;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_RST_CLK_CTRL, data, mask);
+
+	/* Wait for > 55 us to allow PCLK be enabled */
+	udelay(PLL_SET_DELAY_US);
+
+	ret = comphy_lane_reg_poll(lane, COMPHY_PIPE_LANE_STAT1, TXDCLK_PCLK_EN,
+				   COMPHY_PLL_SLEEP, COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to lock USB3 PLL\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static int
+mvebu_a3700_comphy_pcie_power_on(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 mask, data, ref_clk;
+	int ret;
+
+	/* Configure phy selector for PCIe */
+	ret = mvebu_a3700_comphy_set_phy_selector(lane);
+	if (ret)
+		return ret;
+
+	/* 1. Enable max PLL. */
+	comphy_lane_reg_set(lane, COMPHY_PIPE_LANE_CFG1,
+			    USE_MAX_PLL_RATE_EN, USE_MAX_PLL_RATE_EN);
+
+	/* 2. Select 20 bit SERDES interface. */
+	comphy_lane_reg_set(lane, COMPHY_PIPE_CLK_SRC_LO,
+			    CFG_SEL_20B, CFG_SEL_20B);
+
+	/* 3. Force to use reg setting for PCIe mode */
+	comphy_lane_reg_set(lane, COMPHY_MISC_CTRL1,
+			    SEL_BITS_PCIE_FORCE, SEL_BITS_PCIE_FORCE);
+
+	/* 4. Change RX wait */
+	data = CFG_PM_RXDEN_WAIT_1_UNIT | CFG_PM_RXDLOZ_WAIT_12_UNIT;
+	mask = CFG_PM_OSCCLK_WAIT_MASK | CFG_PM_RXDEN_WAIT_MASK |
+	       CFG_PM_RXDLOZ_WAIT_MASK;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_PWR_MGM_TIM1, data, mask);
+
+	/* 5. Enable idle sync */
+	comphy_lane_reg_set(lane, COMPHY_IDLE_SYNC_EN,
+			    IDLE_SYNC_EN, IDLE_SYNC_EN);
+
+	/* 6. Enable the output of 100M/125M/500M clock */
+	data = CLK500M_EN | TXDCLK_2X_SEL | CLK100M_125M_EN;
+	mask = data;
+	comphy_lane_reg_set(lane, COMPHY_MISC_CTRL0, data, mask);
+
+	/*
+	 * 7. Enable TX, PCIE global register, 0xd0074814, it is done in
+	 * PCI-E driver
+	 */
+
+	/*
+	 * 8. Check crystal jumper setting and program the Power and PLL
+	 * Control accordingly
+	 */
+
+	if (lane->priv->xtal_is_40m)
+		ref_clk = REF_FREF_SEL_PCIE_USB3_40MHZ;
+	else
+		ref_clk = REF_FREF_SEL_PCIE_USB3_25MHZ;
+
+	data = PU_IVREF_BIT | PU_PLL_BIT | PU_RX_BIT | PU_TX_BIT |
+	       PU_TX_INTP_BIT | PU_DFE_BIT | COMPHY_MODE_PCIE | ref_clk;
+	mask = 0xFFFF;
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL, data, mask);
+
+	/* 9. Override Speed_PLL value and use MAC PLL */
+	comphy_lane_reg_set(lane, COMPHY_KVCO_CAL_CTRL,
+			    SPEED_PLL_VALUE_16 | USE_MAX_PLL_RATE_BIT,
+			    0xFFFF);
+
+	/* 10. Check the Polarity invert bit */
+	data = 0x0;
+	if (lane->invert_tx)
+		data |= TXD_INVERT_BIT;
+	if (lane->invert_rx)
+		data |= RXD_INVERT_BIT;
+	mask = TXD_INVERT_BIT | RXD_INVERT_BIT;
+	comphy_lane_reg_set(lane, COMPHY_SYNC_PATTERN, data, mask);
+
+	/* 11. Release SW reset */
+	data = MODE_CORE_CLK_FREQ_SEL | MODE_PIPE_WIDTH_32;
+	mask = data | PIPE_SOFT_RESET | MODE_REFDIV_MASK;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_RST_CLK_CTRL, data, mask);
+
+	/* Wait for > 55 us to allow PCLK be enabled */
+	udelay(PLL_SET_DELAY_US);
+
+	ret = comphy_lane_reg_poll(lane, COMPHY_PIPE_LANE_STAT1, TXDCLK_PCLK_EN,
+				   COMPHY_PLL_SLEEP, COMPHY_PLL_TIMEOUT);
+	if (ret) {
+		dev_err(lane->dev, "Failed to lock PCIE PLL\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static void
+mvebu_a3700_comphy_usb3_power_off(struct mvebu_a3700_comphy_lane *lane)
+{
+	/*
+	 * Currently the USB3 MAC sets the USB3 PHY to low state, so we do not
+	 * need to power off USB3 PHY again.
+	 */
+}
+
+static void
+mvebu_a3700_comphy_sata_power_off(struct mvebu_a3700_comphy_lane *lane)
+{
+	/* Set phy isolation mode */
+	comphy_lane_reg_set(lane, COMPHY_ISOLATION_CTRL,
+			    PHY_ISOLATE_MODE, PHY_ISOLATE_MODE);
+
+	/* Power off PLL, Tx, Rx */
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL,
+			    0x0, PU_PLL_BIT | PU_RX_BIT | PU_TX_BIT);
+}
+
+static void
+mvebu_a3700_comphy_ethernet_power_off(struct mvebu_a3700_comphy_lane *lane)
+{
+	u32 mask, data;
+
+	data = PIN_RESET_CORE_BIT | PIN_RESET_COMPHY_BIT | PIN_PU_IVREF_BIT |
+	       PHY_RX_INIT_BIT;
+	mask = data;
+	comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+}
+
+static void
+mvebu_a3700_comphy_pcie_power_off(struct mvebu_a3700_comphy_lane *lane)
+{
+	/* Power off PLL, Tx, Rx */
+	comphy_lane_reg_set(lane, COMPHY_POWER_PLL_CTRL,
+			    0x0, PU_PLL_BIT | PU_RX_BIT | PU_TX_BIT);
+}
+
+static int mvebu_a3700_comphy_reset(struct phy *phy)
+{
+	struct mvebu_a3700_comphy_lane *lane = phy_get_drvdata(phy);
+	u16 mask, data;
+
+	dev_dbg(lane->dev, "resetting lane %d\n", lane->id);
+
+	/* COMPHY reset for internal logic */
+	comphy_lane_reg_set(lane, COMPHY_SFT_RESET,
+			    SFT_RST_NO_REG, SFT_RST_NO_REG);
+
+	/* COMPHY register reset (cleared automatically) */
+	comphy_lane_reg_set(lane, COMPHY_SFT_RESET, SFT_RST, SFT_RST);
+
+	/* PIPE soft and register reset */
+	data = PIPE_SOFT_RESET | PIPE_REG_RESET;
+	mask = data;
+	comphy_lane_reg_set(lane, COMPHY_PIPE_RST_CLK_CTRL, data, mask);
+
+	/* Release PIPE register reset */
+	comphy_lane_reg_set(lane, COMPHY_PIPE_RST_CLK_CTRL,
+			    0x0, PIPE_REG_RESET);
+
+	/* Reset SB configuration register (only for lanes 0 and 1) */
+	if (lane->id == 0 || lane->id == 1) {
+		u32 mask, data;
+
+		data = PIN_RESET_CORE_BIT | PIN_RESET_COMPHY_BIT |
+		       PIN_PU_PLL_BIT | PIN_PU_RX_BIT | PIN_PU_TX_BIT;
+		mask = data | PIN_PU_IVREF_BIT | PIN_TX_IDLE_BIT;
+		comphy_periph_reg_set(lane, COMPHY_PHY_CFG1, data, mask);
+	}
+
+	return 0;
+}
+
+static bool mvebu_a3700_comphy_check_mode(int lane,
 					  enum phy_mode mode,
 					  int submode)
 {
@@ -122,7 +1170,7 @@ static int mvebu_a3700_comphy_get_fw_mod
 
 	/* Unused PHY mux value is 0x0 */
 	if (mode == PHY_MODE_INVALID)
-		return -EINVAL;
+		return false;
 
 	for (i = 0; i < n; i++) {
 		if (mvebu_a3700_comphy_modes[i].lane == lane &&
@@ -132,27 +1180,30 @@ static int mvebu_a3700_comphy_get_fw_mod
 	}
 
 	if (i == n)
-		return -EINVAL;
+		return false;
 
-	return mvebu_a3700_comphy_modes[i].fw_mode;
+	return true;
 }
 
 static int mvebu_a3700_comphy_set_mode(struct phy *phy, enum phy_mode mode,
 				       int submode)
 {
 	struct mvebu_a3700_comphy_lane *lane = phy_get_drvdata(phy);
-	int fw_mode;
-
-	if (submode == PHY_INTERFACE_MODE_1000BASEX)
-		submode = PHY_INTERFACE_MODE_SGMII;
 
-	fw_mode = mvebu_a3700_comphy_get_fw_mode(lane->id, mode,
-						 submode);
-	if (fw_mode < 0) {
+	if (!mvebu_a3700_comphy_check_mode(lane->id, mode, submode)) {
 		dev_err(lane->dev, "invalid COMPHY mode\n");
-		return fw_mode;
+		return -EINVAL;
 	}
 
+	/* Mode cannot be changed while the PHY is powered on */
+	if (phy->power_count &&
+	    (lane->mode != mode || lane->submode != submode))
+		return -EBUSY;
+
+	/* If changing mode, ensure reset is called */
+	if (lane->mode != PHY_MODE_INVALID && lane->mode != mode)
+		lane->needs_reset = true;
+
 	/* Just remember the mode, ->power_on() will do the real setup */
 	lane->mode = mode;
 	lane->submode = submode;
@@ -163,76 +1214,68 @@ static int mvebu_a3700_comphy_set_mode(s
 static int mvebu_a3700_comphy_power_on(struct phy *phy)
 {
 	struct mvebu_a3700_comphy_lane *lane = phy_get_drvdata(phy);
-	u32 fw_param;
-	int fw_mode;
-	int fw_port;
 	int ret;
 
-	fw_mode = mvebu_a3700_comphy_get_fw_mode(lane->id,
-						 lane->mode, lane->submode);
-	if (fw_mode < 0) {
+	if (!mvebu_a3700_comphy_check_mode(lane->id, lane->mode,
+					   lane->submode)) {
 		dev_err(lane->dev, "invalid COMPHY mode\n");
-		return fw_mode;
+		return -EINVAL;
+	}
+
+	if (lane->needs_reset) {
+		ret = mvebu_a3700_comphy_reset(phy);
+		if (ret)
+			return ret;
+
+		lane->needs_reset = false;
 	}
 
 	switch (lane->mode) {
 	case PHY_MODE_USB_HOST_SS:
 		dev_dbg(lane->dev, "set lane %d to USB3 host mode\n", lane->id);
-		fw_param = COMPHY_FW_MODE(fw_mode);
-		break;
+		return mvebu_a3700_comphy_usb3_power_on(lane);
 	case PHY_MODE_SATA:
 		dev_dbg(lane->dev, "set lane %d to SATA mode\n", lane->id);
-		fw_param = COMPHY_FW_MODE(fw_mode);
-		break;
+		return mvebu_a3700_comphy_sata_power_on(lane);
 	case PHY_MODE_ETHERNET:
-		fw_port = (lane->id == 0) ? 1 : 0;
-		switch (lane->submode) {
-		case PHY_INTERFACE_MODE_SGMII:
-			dev_dbg(lane->dev, "set lane %d to SGMII mode\n",
-				lane->id);
-			fw_param = COMPHY_FW_NET(fw_mode, fw_port,
-						 COMPHY_FW_SPEED_1_25G);
-			break;
-		case PHY_INTERFACE_MODE_2500BASEX:
-			dev_dbg(lane->dev, "set lane %d to 2500BASEX mode\n",
-				lane->id);
-			fw_param = COMPHY_FW_NET(fw_mode, fw_port,
-						 COMPHY_FW_SPEED_3_125G);
-			break;
-		default:
-			dev_err(lane->dev, "unsupported PHY submode (%d)\n",
-				lane->submode);
-			return -ENOTSUPP;
-		}
-		break;
+		dev_dbg(lane->dev, "set lane %d to Ethernet mode\n", lane->id);
+		return mvebu_a3700_comphy_ethernet_power_on(lane);
 	case PHY_MODE_PCIE:
 		dev_dbg(lane->dev, "set lane %d to PCIe mode\n", lane->id);
-		fw_param = COMPHY_FW_PCIE(fw_mode, COMPHY_FW_SPEED_5G,
-					  phy->attrs.bus_width);
-		break;
+		return mvebu_a3700_comphy_pcie_power_on(lane);
 	default:
 		dev_err(lane->dev, "unsupported PHY mode (%d)\n", lane->mode);
-		return -ENOTSUPP;
+		return -EOPNOTSUPP;
 	}
-
-	ret = mvebu_a3700_comphy_smc(COMPHY_SIP_POWER_ON, lane->id, fw_param);
-	if (ret == -EOPNOTSUPP)
-		dev_err(lane->dev,
-			"unsupported SMC call, try updating your firmware\n");
-
-	return ret;
 }
 
 static int mvebu_a3700_comphy_power_off(struct phy *phy)
 {
 	struct mvebu_a3700_comphy_lane *lane = phy_get_drvdata(phy);
 
-	return mvebu_a3700_comphy_smc(COMPHY_SIP_POWER_OFF, lane->id, 0);
+	switch (lane->mode) {
+	case PHY_MODE_USB_HOST_SS:
+		mvebu_a3700_comphy_usb3_power_off(lane);
+		return 0;
+	case PHY_MODE_SATA:
+		mvebu_a3700_comphy_sata_power_off(lane);
+		return 0;
+	case PHY_MODE_ETHERNET:
+		mvebu_a3700_comphy_ethernet_power_off(lane);
+		return 0;
+	case PHY_MODE_PCIE:
+		mvebu_a3700_comphy_pcie_power_off(lane);
+		return 0;
+	default:
+		dev_err(lane->dev, "invalid COMPHY mode\n");
+		return -EINVAL;
+	}
 }
 
 static const struct phy_ops mvebu_a3700_comphy_ops = {
 	.power_on	= mvebu_a3700_comphy_power_on,
 	.power_off	= mvebu_a3700_comphy_power_off,
+	.reset		= mvebu_a3700_comphy_reset,
 	.set_mode	= mvebu_a3700_comphy_set_mode,
 	.owner		= THIS_MODULE,
 };
@@ -256,13 +1299,75 @@ static struct phy *mvebu_a3700_comphy_xl
 		return ERR_PTR(-EINVAL);
 	}
 
+	lane->invert_tx = args->args[1] & BIT(0);
+	lane->invert_rx = args->args[1] & BIT(1);
+
 	return phy;
 }
 
 static int mvebu_a3700_comphy_probe(struct platform_device *pdev)
 {
+	struct mvebu_a3700_comphy_priv *priv;
 	struct phy_provider *provider;
 	struct device_node *child;
+	struct resource *res;
+	struct clk *clk;
+	int ret;
+
+	priv = devm_kzalloc(&pdev->dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	spin_lock_init(&priv->lock);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "comphy");
+	priv->comphy_regs = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(priv->comphy_regs))
+		return PTR_ERR(priv->comphy_regs);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+					   "lane1_pcie_gbe");
+	priv->lane1_phy_regs = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(priv->lane1_phy_regs))
+		return PTR_ERR(priv->lane1_phy_regs);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+					   "lane0_usb3_gbe");
+	priv->lane0_phy_regs = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(priv->lane0_phy_regs))
+		return PTR_ERR(priv->lane0_phy_regs);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+					   "lane2_sata_usb3");
+	priv->lane2_phy_indirect = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(priv->lane2_phy_indirect))
+		return PTR_ERR(priv->lane2_phy_indirect);
+
+	/*
+	 * Driver needs to know if reference xtal clock is 40MHz or 25MHz.
+	 * Old DT bindings do not have xtal clk present. So do not fail here
+	 * and expects that default 25MHz reference clock is used.
+	 */
+	clk = clk_get(&pdev->dev, "xtal");
+	if (IS_ERR(clk)) {
+		if (PTR_ERR(clk) == -EPROBE_DEFER)
+			return -EPROBE_DEFER;
+		dev_warn(&pdev->dev, "missing 'xtal' clk (%ld)\n",
+			 PTR_ERR(clk));
+	} else {
+		ret = clk_prepare_enable(clk);
+		if (ret) {
+			dev_warn(&pdev->dev, "enabling xtal clk failed (%d)\n",
+				 ret);
+		} else {
+			if (clk_get_rate(clk) == 40000000)
+				priv->xtal_is_40m = true;
+			clk_disable_unprepare(clk);
+		}
+		clk_put(clk);
+	}
+
+	dev_set_drvdata(&pdev->dev, priv);
 
 	for_each_available_child_of_node(pdev->dev.of_node, child) {
 		struct mvebu_a3700_comphy_lane *lane;
@@ -277,7 +1382,7 @@ static int mvebu_a3700_comphy_probe(stru
 			continue;
 		}
 
-		if (lane_id >= MVEBU_A3700_COMPHY_LANES) {
+		if (lane_id >= 3) {
 			dev_err(&pdev->dev, "invalid 'reg' property\n");
 			continue;
 		}
@@ -295,11 +1400,21 @@ static int mvebu_a3700_comphy_probe(stru
 			return PTR_ERR(phy);
 		}
 
+		lane->priv = priv;
 		lane->dev = &pdev->dev;
 		lane->mode = PHY_MODE_INVALID;
 		lane->submode = PHY_INTERFACE_MODE_NA;
 		lane->id = lane_id;
+		lane->invert_tx = false;
+		lane->invert_rx = false;
 		phy_set_drvdata(phy, lane);
+
+		/*
+		 * To avoid relying on the bootloader/firmware configuration,
+		 * power off all comphys.
+		 */
+		mvebu_a3700_comphy_reset(phy);
+		lane->needs_reset = false;
 	}
 
 	provider = devm_of_phy_provider_register(&pdev->dev,
@@ -323,5 +1438,7 @@ static struct platform_driver mvebu_a370
 module_platform_driver(mvebu_a3700_comphy_driver);
 
 MODULE_AUTHOR("Miquèl Raynal <miquel.raynal@bootlin.com>");
+MODULE_AUTHOR("Pali Rohár <pali@kernel.org>");
+MODULE_AUTHOR("Marek Behún <kabel@kernel.org>");
 MODULE_DESCRIPTION("Common PHY driver for A3700");
 MODULE_LICENSE("GPL v2");
