// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Buffalo WXR-2533DHP";
	compatible = "buffalo,wxr-2533dhp", "qcom,ipq8064";

	memory@42000000 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &diag;
		led-running = &power;
		led-upgrade = &power;
	};

	chosen {
		/* use "ubi_rootfs" volume in "ubi" partition as rootfs */
		bootargs = "ubi.block=0,1 root=/dev/ubiblock0_1 rootfstype=squashfs";
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		usb {
			label = "green:usb";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "usbport";
			trigger-sources = <&hub_port0 &hub_port1>;
		};

		guestport {
			label = "green:guestport";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		diag: diag {
			label = "orange:diag";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		internet_orange {
			label = "orange:internet";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_HIGH>;
		};

		internet_white {
			label = "white:internet";
			gpios = <&qcom_pinmux 22 GPIO_ACTIVE_HIGH>;
		};

		wireless_orange {
			label = "orange:wireless";
			gpios = <&qcom_pinmux 23 GPIO_ACTIVE_HIGH>;
		};

		wireless_white {
			label = "white:wireless";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_HIGH>;
		};

		router_orange {
			label = "orange:router";
			gpios = <&qcom_pinmux 25 GPIO_ACTIVE_HIGH>;
		};

		router_white {
			label = "white:router";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_LOW>;
		};

		power: power {
			label = "white:power";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		power {
			label = "power";
			gpios = <&qcom_pinmux 58 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		eject {
			label = "eject";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_EJECTCD>;
			debounce-interval = <60>;
			wakeup-source;
		};

		guest {
			label = "guest";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			debounce-interval = <60>;
			wakeup-source;
		};

		ap {
			label = "ap";
			gpios = <&qcom_pinmux 55 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};

		router {
			label = "router";
			gpios = <&qcom_pinmux 56 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};

		auto {
			label = "auto";
			gpios = <&qcom_pinmux 57 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};
};

&nand_controller {
	status = "okay";

	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";

	cs@0 {
		reg = <0>;
		compatible = "qcom,nandcs";

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			ubi@0 {
				label = "ubi";
				reg = <0x0000000 0x4000000>;
			};

			rootfs_1@4000000 {
				label = "rootfs_1";
				reg = <0x4000000 0x4000000>;
			};
		};
	};
};

&adm_dma {
	status = "okay";
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	ethernet-phy@0 {
		reg = <0>;
		qca,ar8327-initvals = <
			0x00004 0x07600000  /* PAD0_MODE */
			0x00008 0x01000000  /* PAD5_MODE */
			0x0000c 0x00000080  /* PAD6_MODE */
			0x00050 0xcc35cc35  /* LED_CTRL0 */
			0x00054 0xca35ca35  /* LED_CTRL1 */
			0x00058 0xc935c935  /* LED_CTRL2 */
			0x0005c 0x03ffff00  /* LED_CTRL3 */
			0x000e4 0x0006a545  /* MAC_POWER_SEL */
			0x000e0 0xc74164de  /* SGMII_CTRL */
			0x0007c 0x0000007e  /* PORT0_STATUS */
			0x00094 0x0000007e  /* PORT6_STATUS */
			>;
	};

	ethernet-phy@4 {
		reg = <4>;
	};
};

&gmac1 {
	status = "okay";

	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_ART_6>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";

	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_ART_0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gsbi4_serial {
	pinctrl-0 = <&uart0_pins>;
	pinctrl-names = "default";
};

&gsbi5 {
	status = "okay";
	qcom,mode = <GSBI_PROT_SPI>;

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		flash@0 {
			compatible = "jedec,spi-nor";
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				SBL1@0 {
					label = "SBL1";
					reg = <0x0 0x10000>;
					read-only;
				};

				MIBIB@10000 {
					label = "MIBIB";
					reg = <0x10000 0x20000>;
					read-only;
				};

				SBL2@30000 {
					label = "SBL2";
					reg = <0x30000 0x30000>;
					read-only;
				};

				SBL3@60000 {
					label = "SBL3";
					reg = <0x60000 0x30000>;
					read-only;
				};

				DDRCONFIG@90000 {
					label = "DDRCONFIG";
					reg = <0x90000 0x10000>;
					read-only;
				};

				SSD@a0000 {
					label = "SSD";
					reg = <0xa0000 0x10000>;
					read-only;
				};

				TZ@b0000 {
					label = "TZ";
					reg = <0xb0000 0x30000>;
					read-only;
				};

				RPM@e0000 {
					label = "RPM";
					reg = <0xe0000 0x20000>;
					read-only;
				};

				APPSBL@100000 {
					label = "APPSBL";
					reg = <0x100000 0x70000>;
					read-only;
				};

				APPSBLENV@170000 {
					label = "APPSBLENV";
					reg = <0x170000 0x10000>;
					read-only;
				};

				ART@180000 {
					label = "ART";
					reg = <0x180000 0x40000>;
					read-only;

					compatible = "nvmem-cells";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_ART_0: macaddr@0 {
						reg = <0x0 0x6>;
					};

					macaddr_ART_6: macaddr@6 {
						reg = <0x6 0x6>;
					};

					macaddr_ART_18: macaddr@18 {
						reg = <0x18 0x6>;
					};

					macaddr_ART_1e: macaddr@1e {
						reg = <0x1e 0x6>;
					};

					precal_ART_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_ART_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};

				BOOTCONFIG@1c0000 {
					label = "BOOTCONFIG";
					reg = <0x1c0000 0x10000>;
					read-only;
				};

				APPSBL_1@1d0000 {
					label = "APPSBL_1";
					reg = <0x1d0000 0x70000>;
					read-only;
				};
			};
		};
	};
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb_pwr_en_pins>;
	pinctrl-names = "default";
};

&usb3_1 {
	status = "okay";
};

&dwc3_0 {
	#address-cells = <1>;
	#size-cells = <0>;

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&dwc3_1 {
	#address-cells = <1>;
	#size-cells = <0>;

	hub_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&pcie0 {
	status = "okay";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_ART_1e>, <&precal_ART_1000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&pcie1 {
	status = "okay";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_ART_18>, <&precal_ART_5000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio6", "gpio54", "gpio55", "gpio56", "gpio57",
				"gpio58", "gpio64", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8", "gpio9", "gpio16", "gpio22",
				"gpio23", "gpio24", "gpio25", "gpio26", "gpio53";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	uart0_pins: uart0_pins {
		mux {
			pins = "gpio10", "gpio11";
			function = "gsbi4";
			drive-strength = <12>;
			bias-disable;
		};
	};

	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs{
			pins = "gpio20";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};

	usb_pwr_en_pins: usb_pwr_en_pins {
		mux{
			pins = "gpio68";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
			output-high;
		};
	};
};
