From: Johannes Berg <johannes.berg@intel.com>
Date: Wed, 28 Sep 2022 22:01:37 +0200
Subject: [PATCH] wifi: cfg80211/mac80211: reject bad MBSSID elements

commit 8f033d2becc24aa6bfd2a5c104407963560caabc upstream

Per spec, the maximum value for the MaxBSSID ('n') indicator is 8,
and the minimum is 1 since a multiple BSSID set with just one BSSID
doesn't make sense (the # of BSSIDs is limited by 2^n).

Limit this in the parsing in both cfg80211 and mac80211, rejecting
any elements with an invalid value.

This fixes potentially bad shifts in the processing of these inside
the cfg80211_gen_new_bssid() function later.

I found this during the investigation of CVE-2022-41674 fixed by the
previous patch.

Fixes: 0b8fb8235be8 ("cfg80211: Parsing of Multiple BSSID information in scanning")
Fixes: 78ac51f81532 ("mac80211: support multi-bssid")
Reviewed-by: Kees Cook <keescook@chromium.org>
Signed-off-by: Johannes Berg <johannes.berg@intel.com>
---

--- a/net/mac80211/util.c
+++ b/net/mac80211/util.c
@@ -1413,6 +1413,8 @@ static size_t ieee802_11_find_bssid_prof
 	for_each_element_id(elem, WLAN_EID_MULTIPLE_BSSID, start, len) {
 		if (elem->datalen < 2)
 			continue;
+		if (elem->data[0] < 1 || elem->data[0] > 8)
+			continue;
 
 		for_each_element(sub, elem->data + 1, elem->datalen - 1) {
 			u8 new_bssid[ETH_ALEN];
--- a/net/wireless/scan.c
+++ b/net/wireless/scan.c
@@ -2103,6 +2103,8 @@ static void cfg80211_parse_mbssid_data(s
 	for_each_element_id(elem, WLAN_EID_MULTIPLE_BSSID, ie, ielen) {
 		if (elem->datalen < 4)
 			continue;
+		if (elem->data[0] < 1 || (int)elem->data[0] > 8)
+			continue;
 		for_each_element(sub, elem->data + 1, elem->datalen - 1) {
 			u8 profile_len;
 
