From fed7cef5e4f2df8c6a79bebf5da1fdd3783ff6f3 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Mon, 4 Jul 2022 13:36:22 +0200
Subject: [PATCH] ARM: dts: turris-omnia: enable LED controller node
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The LED controller node is disabled because the leds-turris-omnia driver
does not support setting the LED blinking to be controlled by the MCU.

The patches for that have now been sent [1], so let's enable the node.

[1] https://lore.kernel.org/linux-leds/20220704105955.15474-1-kabel@kernel.org/T/

Signed-off-by: Marek Behún <kabel@kernel.org>
---
 arch/arm/boot/dts/armada-385-turris-omnia.dts | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/armada-385-turris-omnia.dts
+++ b/arch/arm/boot/dts/armada-385-turris-omnia.dts
@@ -189,15 +189,13 @@
 				reg = <0x2b>;
 				#address-cells = <1>;
 				#size-cells = <0>;
+				status = "okay";
 
 				/*
 				 * LEDs are controlled by MCU (STM32F0) at
 				 * address 0x2b.
 				 *
-				 * The driver does not support HW control mode
-				 * for the LEDs yet. Disable the LEDs for now.
-				 *
-				 * Also LED functions are not stable yet:
+				 * LED functions are not stable yet:
 				 * - there are 3 LEDs connected via MCU to PCIe
 				 *   ports. One of these ports supports mSATA.
 				 *   There is no mSATA nor PCIe function.
@@ -208,7 +206,6 @@
 				 *   B. Again there is no such function defined.
 				 *   For now we use LED_FUNCTION_INDICATOR
 				 */
-				status = "disabled";
 
 				multi-led@0 {
 					reg = <0x0>;
