From 1c6c1ab42e61cdca555c85bdde5677b13b5cd5f3 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Fri, 6 Sep 2019 15:04:51 +0100
Subject: [PATCH] v4l2: Add a Greyworld AWB mode.

Adds a simple greyworld white balance preset, mainly for use
with cameras without an IR filter (eg Raspberry Pi NoIR)

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/media/v4l2-core/v4l2-ctrls.c | 1 +
 include/uapi/linux/v4l2-controls.h   | 1 +
 2 files changed, 2 insertions(+)

--- a/drivers/media/v4l2-core/v4l2-ctrls.c
+++ b/drivers/media/v4l2-core/v4l2-ctrls.c
@@ -275,6 +275,7 @@ const char * const *v4l2_ctrl_get_menu(u
 		"Flash",
 		"Cloudy",
 		"Shade",
+		"Greyworld",
 		NULL,
 	};
 	static const char * const camera_iso_sensitivity_auto[] = {
--- a/include/uapi/linux/v4l2-controls.h
+++ b/include/uapi/linux/v4l2-controls.h
@@ -886,6 +886,7 @@ enum v4l2_auto_n_preset_white_balance {
 	V4L2_WHITE_BALANCE_FLASH		= 7,
 	V4L2_WHITE_BALANCE_CLOUDY		= 8,
 	V4L2_WHITE_BALANCE_SHADE		= 9,
+	V4L2_WHITE_BALANCE_GREYWORLD		= 10,
 };
 
 #define V4L2_CID_WIDE_DYNAMIC_RANGE		(V4L2_CID_CAMERA_CLASS_BASE+21)
