From patchwork Sat Sep 17 20:27:56 2022
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 12979248
X-Patchwork-Delegate: kvalo@adurom.com
Return-Path: <linux-wireless-owner@kernel.org>
Date: Sat, 17 Sep 2022 21:27:56 +0100
From: Daniel Golle <daniel@makrotopia.org>
To: linux-wireless@vger.kernel.org, Stanislaw Gruszka <stf_xl@wp.pl>,
        Helmut Schaa <helmut.schaa@googlemail.com>
Cc: Kalle Valo <kvalo@kernel.org>,
        "David S. Miller" <davem@davemloft.net>,
        Eric Dumazet <edumazet@google.com>,
        Jakub Kicinski <kuba@kernel.org>,
        Paolo Abeni <pabeni@redhat.com>,
        Johannes Berg <johannes.berg@intel.com>
Subject: [PATCH v3 07/16] rt2x00: add RXDCOC calibration for MT7620
Message-ID: 
 <850b30f652e88de30d79e968af4eb47aa5bc2511.1663445157.git.daniel@makrotopia.org>
References: <cover.1663445157.git.daniel@makrotopia.org>
MIME-Version: 1.0
Content-Disposition: inline
In-Reply-To: <cover.1663445157.git.daniel@makrotopia.org>
Precedence: bulk
List-ID: <linux-wireless.vger.kernel.org>
X-Mailing-List: linux-wireless@vger.kernel.org

From: Tomislav Požega <pozega.tomislav@gmail.com>

Add RXDCOC calibration code from mtk driver.

Signed-off-by: Tomislav Požega <pozega.tomislav@gmail.com>
[fixed typo reported by Serge Vasilugin <vasilugin@yandex.ru>]
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Acked-by: Stanislaw Gruszka <stf_xl@wp.pl>
---
 .../net/wireless/ralink/rt2x00/rt2800lib.c    | 60 +++++++++++++++++++
 1 file changed, 60 insertions(+)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -8607,6 +8607,65 @@ static void rt2800_r_calibration(struct
 	rt2800_register_write(rt2x00dev, PWR_PIN_CFG, MAC_PWR_PIN_CFG);
 }
 
+static void rt2800_rxdcoc_calibration(struct rt2x00_dev *rt2x00dev)
+{
+	u8 bbpreg = 0;
+	u32 macvalue = 0;
+	u8 saverfb0r2, saverfb5r4, saverfb7r4, rfvalue;
+	int i;
+
+	saverfb0r2 = rt2800_rfcsr_read_bank(rt2x00dev, 0, 2);
+	rfvalue = saverfb0r2;
+	rfvalue |= 0x03;
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 2, rfvalue);
+
+	rt2800_bbp_write(rt2x00dev, 158, 141);
+	bbpreg = rt2800_bbp_read(rt2x00dev, 159);
+	bbpreg |= 0x10;
+	rt2800_bbp_write(rt2x00dev, 159, bbpreg);
+
+	macvalue = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, 0x8);
+
+	if (unlikely(rt2800_wait_bbp_rf_ready(rt2x00dev, MAC_STATUS_CFG_BBP_RF_BUSY_TX)))
+		rt2x00_warn(rt2x00dev, "RF TX busy in RX RXDCOC calibration\n");
+
+	saverfb5r4 = rt2800_rfcsr_read_bank(rt2x00dev, 5, 4);
+	saverfb7r4 = rt2800_rfcsr_read_bank(rt2x00dev, 7, 4);
+	saverfb5r4 = saverfb5r4 & (~0x40);
+	saverfb7r4 = saverfb7r4 & (~0x40);
+	rt2800_rfcsr_write_dccal(rt2x00dev, 4, 0x64);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 4, saverfb5r4);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 4, saverfb7r4);
+
+	rt2800_bbp_write(rt2x00dev, 158, 141);
+	bbpreg = rt2800_bbp_read(rt2x00dev, 159);
+	bbpreg = bbpreg & (~0x40);
+	rt2800_bbp_write(rt2x00dev, 159, bbpreg);
+	bbpreg |= 0x48;
+	rt2800_bbp_write(rt2x00dev, 159, bbpreg);
+
+	for (i = 0; i < 10000; i++) {
+		bbpreg = rt2800_bbp_read(rt2x00dev, 159);
+		if ((bbpreg & 0x40) == 0)
+			break;
+		usleep_range(50, 100);
+	}
+
+	bbpreg = rt2800_bbp_read(rt2x00dev, 159);
+	bbpreg = bbpreg & (~0x40);
+	rt2800_bbp_write(rt2x00dev, 159, bbpreg);
+
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, macvalue);
+
+	rt2800_bbp_write(rt2x00dev, 158, 141);
+	bbpreg = rt2800_bbp_read(rt2x00dev, 159);
+	bbpreg &= (~0x10);
+	rt2800_bbp_write(rt2x00dev, 159, bbpreg);
+
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 2, saverfb0r2);
+}
+
 static void rt2800_bbp_core_soft_reset(struct rt2x00_dev *rt2x00dev,
 				       bool set_bw, bool is_ht40)
 {
@@ -9216,6 +9275,7 @@ static void rt2800_init_rfcsr_6352(struc
 
 	rt2800_r_calibration(rt2x00dev);
 	rt2800_rf_self_txdc_cal(rt2x00dev);
+	rt2800_rxdcoc_calibration(rt2x00dev);
 	rt2800_bw_filter_calibration(rt2x00dev, true);
 	rt2800_bw_filter_calibration(rt2x00dev, false);
 }
