From: Gabor Juhos <juhosg@openwrt.org>
Subject: kernel/3.1[02]: move MTD root device setup code to mtdcore

The current code only allows to automatically set
root device on MTD partitions. Move the code to MTD
core to allow to use it with all MTD devices.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/mtd/mtdcore.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -27,6 +27,7 @@
 #include <linux/reboot.h>
 #include <linux/leds.h>
 #include <linux/debugfs.h>
+#include <linux/root_dev.h>
 #include <linux/nvmem-provider.h>
 
 #include <linux/mtd/mtd.h>
@@ -767,6 +768,19 @@ int add_mtd_device(struct mtd_info *mtd)
 	   of this try_ nonsense, and no bitching about it
 	   either. :) */
 	__module_get(THIS_MODULE);
+
+	if (!strcmp(mtd->name, "rootfs") &&
+	    IS_ENABLED(CONFIG_MTD_ROOTFS_ROOT_DEV) &&
+	    ROOT_DEV == 0) {
+		unsigned int index = mtd->index;
+		pr_notice("mtd: device %d (%s) set to be root filesystem\n",
+			  mtd->index, mtd->name);
+#ifdef CONFIG_FIT_PARTITION
+		index <<= 2;
+#endif
+		ROOT_DEV = MKDEV(MTD_BLOCK_MAJOR, index);
+	}
+
 	return 0;
 
 fail_nvmem_add:
