// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "oraybox,x3a", "mediatek,mt7621-soc";
	model = "OrayBox X3A";

	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-running = &led_status_blue;
		led-upgrade = &led_status_green;
		label-mac-device = &gmac0;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		led_status_red: status-red {
			label = "red:status";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_status_blue: status-blue {
			label = "blue:status";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led_status_green: status-green {
			label = "green:status";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <30000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xf00000>;
			};

			partition@fe0000 {
				label = "bdinfo";
				reg = <0xfe0000 0x10000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_bdinfo_9: macaddr@9 {
					reg = <0x9 0x6>;
				};
			};

			partition@ff0000 {
				label = "reserve";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_bdinfo_9>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {		
		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};

		port@4 {
			status = "okay";
			label = "wan";
			nvmem-cells = <&macaddr_bdinfo_9>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <1>;
		};
	};
};

&state_default {
	gpio {
		groups = "jtag", "wdt";
		function = "gpio";
	};
};
