From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 18 Jul 2022 13:16:05 +0200
Subject: [PATCH] arm64: dts: broadcom: bcm4908: add remaining LED pins
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Include all 32 pins.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 .../boot/dts/broadcom/bcm4908/bcm4908.dtsi    | 75 +++++++++++++++++++
 1 file changed, 75 insertions(+)

--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
@@ -352,6 +352,61 @@
 				groups = "led_9_grp_a";
 			};
 
+			pins_led_10_a: led_10-a-pins {
+				function = "led_10";
+				groups = "led_10_grp_a";
+			};
+
+			pins_led_11_a: led_11-a-pins {
+				function = "led_11";
+				groups = "led_11_grp_a";
+			};
+
+			pins_led_12_a: led_12-a-pins {
+				function = "led_12";
+				groups = "led_12_grp_a";
+			};
+
+			pins_led_13_a: led_13-a-pins {
+				function = "led_13";
+				groups = "led_13_grp_a";
+			};
+
+			pins_led_14_a: led_14-a-pins {
+				function = "led_14";
+				groups = "led_14_grp_a";
+			};
+
+			pins_led_15_a: led_15-a-pins {
+				function = "led_15";
+				groups = "led_15_grp_a";
+			};
+
+			pins_led_16_a: led_16-a-pins {
+				function = "led_16";
+				groups = "led_16_grp_a";
+			};
+
+			pins_led_17_a: led_17-a-pins {
+				function = "led_17";
+				groups = "led_17_grp_a";
+			};
+
+			pins_led_18_a: led_18-a-pins {
+				function = "led_18";
+				groups = "led_18_grp_a";
+			};
+
+			pins_led_19_a: led_19-a-pins {
+				function = "led_19";
+				groups = "led_19_grp_a";
+			};
+
+			pins_led_20_a: led_20-a-pins {
+				function = "led_20";
+				groups = "led_20_grp_a";
+			};
+
 			pins_led_21_a: led_21-a-pins {
 				function = "led_21";
 				groups = "led_21_grp_a";
@@ -362,6 +417,21 @@
 				groups = "led_22_grp_a";
 			};
 
+			pins_led_23_a: led_23-a-pins {
+				function = "led_23";
+				groups = "led_23_grp_a";
+			};
+
+			pins_led_24_a: led_24-a-pins {
+				function = "led_24";
+				groups = "led_24_grp_a";
+			};
+
+			pins_led_25_a: led_25-a-pins {
+				function = "led_25";
+				groups = "led_25_grp_a";
+			};
+
 			pins_led_26_a: led_26-a-pins {
 				function = "led_26";
 				groups = "led_26_grp_a";
@@ -387,6 +457,11 @@
 				groups = "led_30_grp_a";
 			};
 
+			pins_led_31_a: led_31-a-pins {
+				function = "led_31";
+				groups = "led_31_grp_a";
+			};
+
 			pins_hs_uart: hs_uart-pins {
 				function = "hs_uart";
 				groups = "hs_uart_grp";
