From 8c11d9b768c6753f045e8669a9d90bb008874b4b Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Wed, 9 Dec 2020 16:37:01 +0000
Subject: [PATCH] bcm2711: Disable bsc_intr and aon_intr by default and
 enable in overlay

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 arch/arm/boot/dts/bcm2711.dtsi                     |  2 ++
 .../boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts  | 14 ++++++++++++++
 2 files changed, 16 insertions(+)

--- a/arch/arm/boot/dts/bcm2711.dtsi
+++ b/arch/arm/boot/dts/bcm2711.dtsi
@@ -315,6 +315,7 @@
 			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			interrupt-controller;
 			#interrupt-cells = <1>;
+			status = "disabled";
 		};
 
 		hdmi0: hdmi@7ef00700 {
--- a/arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts
+++ b/arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts
@@ -166,6 +166,13 @@
 		};
 	};
 
+	fragment@24 {
+		target = <&aon_intr>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
 	__overrides__ {
 		audio   = <0>,"!17";
 		audio1   = <0>,"!18";
