From 3774310df4996e7ce45854ddb47a6cf969295f9d Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 31 Oct 2018 14:55:37 +0000
Subject: [PATCH] media: ov5647: Add set_fmt and get_fmt calls.

There's no way to query the subdevice for the supported
resolutions.
Add set_fmt and get_fmt implementations.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/media/i2c/ov5647.c | 22 ++++++++++++++++++++++
 1 file changed, 22 insertions(+)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -463,8 +463,30 @@ static int ov5647_enum_mbus_code(struct
 	return 0;
 }
 
+static int ov5647_set_get_fmt(struct v4l2_subdev *sd,
+			      struct v4l2_subdev_pad_config *cfg,
+			      struct v4l2_subdev_format *format)
+{
+	struct v4l2_mbus_framefmt *fmt = &format->format;
+
+	if (format->pad != 0)
+		return -EINVAL;
+
+	/* Only one format is supported, so return that */
+	memset(fmt, 0, sizeof(*fmt));
+	fmt->code = MEDIA_BUS_FMT_SBGGR8_1X8;
+	fmt->colorspace = V4L2_COLORSPACE_SRGB;
+	fmt->field = V4L2_FIELD_NONE;
+	fmt->width = 640;
+	fmt->height = 480;
+
+	return 0;
+}
+
 static const struct v4l2_subdev_pad_ops ov5647_subdev_pad_ops = {
 	.enum_mbus_code = ov5647_enum_mbus_code,
+	.set_fmt =	  ov5647_set_get_fmt,
+	.get_fmt =	  ov5647_set_get_fmt,
 };
 
 static const struct v4l2_subdev_ops ov5647_subdev_ops = {
