From 8c9e8b0a28225c46f2cca0a09a3a111bb043e874 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 17 Jun 2020 12:50:41 +0200
Subject: [PATCH 9/9] mips: bmips: add BCM6318 reset controller definitions
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM6318 SoCs have a reset controller for certain components.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Acked-by: Florian Fainelli <F.fainelli@gmail.com>
Reviewed-by: Rob Herring <robh@kernel.org>
Signed-off-by: Thomas Bogendoerfer <tsbogend@alpha.franken.de>
---
 include/dt-bindings/reset/bcm6318-reset.h | 20 ++++++++++++++++++++
 1 file changed, 20 insertions(+)
 create mode 100644 include/dt-bindings/reset/bcm6318-reset.h

--- /dev/null
+++ b/include/dt-bindings/reset/bcm6318-reset.h
@@ -0,0 +1,20 @@
+/* SPDX-License-Identifier: GPL-2.0+ */
+
+#ifndef __DT_BINDINGS_RESET_BCM6318_H
+#define __DT_BINDINGS_RESET_BCM6318_H
+
+#define BCM6318_RST_SPI		0
+#define BCM6318_RST_EPHY	1
+#define BCM6318_RST_SAR		2
+#define BCM6318_RST_ENETSW	3
+#define BCM6318_RST_USBD	4
+#define BCM6318_RST_USBH	5
+#define BCM6318_RST_PCIE_CORE	6
+#define BCM6318_RST_PCIE	7
+#define BCM6318_RST_PCIE_EXT	8
+#define BCM6318_RST_PCIE_HARD	9
+#define BCM6318_RST_ADSL	10
+#define BCM6318_RST_PHYMIPS	11
+#define BCM6318_RST_HOSTMIPS	12
+
+#endif /* __DT_BINDINGS_RESET_BCM6318_H */
