From c86a9763861a14dd1d9cc21338136b50b6797321 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 9 Jan 2024 18:44:49 +0000
Subject: [PATCH 1061/1085] drm/bridge: tc358762: revert move ops to enable

Reverts 8a4b2fc9c91a ("drm/bridge: tc358762: Split register programming from pre-enable to enable")
as we want the config commands sent before video starts.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/bridge/tc358762.c | 9 ---------
 1 file changed, 9 deletions(-)

--- a/drivers/gpu/drm/bridge/tc358762.c
+++ b/drivers/gpu/drm/bridge/tc358762.c
@@ -200,14 +200,6 @@ static void tc358762_pre_enable(struct d
 		usleep_range(5000, 10000);
 	}
 
-	ctx->pre_enabled = true;
-}
-
-static void tc358762_enable(struct drm_bridge *bridge, struct drm_bridge_state *state)
-{
-	struct tc358762 *ctx = bridge_to_tc358762(bridge);
-	int ret;
-
 	ret = tc358762_init(ctx);
 	if (ret < 0)
 		dev_err(ctx->dev, "error initializing bridge (%d)\n", ret);
@@ -234,7 +226,6 @@ static void tc358762_bridge_mode_set(str
 static const struct drm_bridge_funcs tc358762_bridge_funcs = {
 	.atomic_post_disable = tc358762_post_disable,
 	.atomic_pre_enable = tc358762_pre_enable,
-	.atomic_enable = tc358762_enable,
 	.atomic_duplicate_state = drm_atomic_helper_bridge_duplicate_state,
 	.atomic_destroy_state = drm_atomic_helper_bridge_destroy_state,
 	.atomic_reset = drm_atomic_helper_bridge_reset,
