From fa9b3bdb56e69dc21d449d041518f8ba58563823 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 6 Nov 2019 13:57:58 +0000
Subject: [PATCH 0185/1085] staging: vchiq_arm: Register bcm2835-codec as a
 platform driver

Following the same pattern as bcm2835-camera and bcm2835-audio,
register the V4L2 codec driver as a platform driver

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
+++ b/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -67,6 +67,7 @@ struct vchiq_state g_state;
 
 static struct platform_device *bcm2835_camera;
 static struct platform_device *bcm2835_audio;
+static struct platform_device *bcm2835_codec;
 static struct platform_device *vcsm_cma;
 
 struct vchiq_drvdata {
@@ -1827,6 +1828,7 @@ static int vchiq_probe(struct platform_d
 	}
 
 	vcsm_cma = vchiq_register_child(pdev, "vcsm-cma");
+	bcm2835_codec = vchiq_register_child(pdev, "bcm2835-codec");
 	bcm2835_camera = vchiq_register_child(pdev, "bcm2835-camera");
 	bcm2835_audio = vchiq_register_child(pdev, "bcm2835_audio");
 
@@ -1842,6 +1844,7 @@ static void vchiq_remove(struct platform
 {
 	platform_device_unregister(bcm2835_audio);
 	platform_device_unregister(bcm2835_camera);
+	platform_device_unregister(bcm2835_codec);
 	platform_device_unregister(vcsm_cma);
 	vchiq_debugfs_deinit();
 	vchiq_deregister_chrdev();
