#include "mt7622-ubnt-unifi-6-lr.dtsi"

/ {
	aliases {
		led-boot = &led_white;
		led-failsafe = &led_white;
		led-running = &led_blue;
		led-upgrade = &led_blue;
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_white: dome_white {
			label = "white:dome";
			gpios = <&pio 0x43 GPIO_ACTIVE_LOW>;
		};

		led_blue: dome_blue {
			label = "blue:dome";
			gpios = <&pio 0x44 GPIO_ACTIVE_HIGH>;
		};
	};
};

&eth {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&eth_pins>;

	gmac0: mac@0 {
		compatible = "mediatek,eth-mac";
		reg = <0>;

		phy-mode = "2500base-x";
		phy-handle = <&phy0>;
		phy-connection-type = "2500base-x";
	};

	mdio: mdio-bus {
		#address-cells = <1>;
		#size-cells = <0>;

		phy0: ethernet-phy@8 {
			compatible = "ethernet-phy-ieee802.3-c45";
			reg = <0x8>;
		};
	};
};

